//
// (c)2004 GE Medical Systems
//
// Description:
//       Dicom dictionary, containing
//			- DICOM 2000 part 6 (MJS)
//			- some supplement (JPD)
//
DATA_ELEM(0000, 0002, UI, "Affected SOP Class UID") // The affected SOP Class UID associated with the operation.
DATA_ELEM(0000, 0003, UI, "Requested SOP Class UID") // The requested SOP Class UID associated with the operation.
DATA_ELEM(0000, 0100, US, "Command Field") // This field distinguishes the DIMSE operation conveyed by this Message. This field shall be set to one of the following values: 0001H C-SEND-RQ 8001H C-SEND-RSP 0010H C-GET-RQ 8010H C-GET-RSP 0020H C-FIND-RQ 8020H C-FIND-RSP 0021H C-MOVE-RQ 8021H C-MOVE-RSP 0030H C-ECHO-RQ 8030H C-ECHO-RSP 0100H N-EVENT-REPORT-RQ 8100H N-EVENT-REPORT-RSP 0110H N-GET-RQ 8110H N-GET-RSP 0120H N-SET-RQ 8120H N-SET-RSP 0130H N-ACTION-RQ 8130H N-ACTION-RSP 0140H N-CREATE-RQ 8140H N-CREATE-RSP 0150H N-DELETE-RQ 8150H N-DELETE-RSP 0FFFH C-CANCEL-RQ
DATA_ELEM(0000, 0110, US, "Message ID") // Implementation-specific value which distinguishes this Message from other Messages.
DATA_ELEM(0000, 0120, US, "Message ID Being Responded To") // Shall be set to the value of the Message ID (0000,0110) field used in associated request Message.
DATA_ELEM(0000, 0600, AE, "Move Destination") // Shall be set to the DICOM AE Title of the destination DICOM AE for which the C-STORE sub-operations are being performed.
DATA_ELEM(0000, 0700, US, "Priority") // The priority shall be set to one of the following values: LOW = 0002H MEDIUM = 0000H HIGH = 0001H
DATA_ELEM(0000, 0800, US, "Data Set Type") // This field indicates if a Data Set is present in the Message. This field shall be set to the value of 0101H if no Data Set is present; any other value indicates a Data Set is included in the Message.
DATA_ELEM(0000, 0900, US, "Status") // Confirmation status of the operation. See Annex C.
DATA_ELEM(0000, 0901, AT, "Offending Element") // If status is Cxxx, then this field contains a list of the elements in which the error was detected.
DATA_ELEM(0000, 0902, LO, "Error Comment") // This field contains an application-specific text description of the error detected.
DATA_ELEM(0000, 0903, US, "Error ID") // This field shall optionally contain an application-specific error code.
DATA_ELEM(0000, 1000, UI, "Affected SOP Instance UID") // Contains the UID of the SOP Instance for which this operation occurred.
DATA_ELEM(0000, 1001, UI, "Requested SOP Instance UID") // Contains the UID of the SOP Instance for which this operation occurred.
DATA_ELEM(0000, 1002, US, "Event Type ID") // Values for this field are application-specific.
DATA_ELEM(0000, 1005, AT, "Attribute Identifier List") // This field contains an Attribute Tag for each of the n Attributes applicable.
DATA_ELEM(0000, 1008, US, "Action Type ID") // Values for this field are application-specific.
DATA_ELEM(0000, 1020, US, "Number of Remaining Sub-operations") // The number of remaining C-STORE sub-operations to be invoked for the operation.
DATA_ELEM(0000, 1021, US, "Number of Completed Sub-operations") // The number of C-STORE sub-operations associated with this operation which have completed successfully.
DATA_ELEM(0000, 1022, US, "Number of Failed Sub-operations") // The number of C-STORE sub-operations associated with this operation which have failed.
DATA_ELEM(0000, 1023, US, "Number of Warning Sub-operations") // The number of C-STORE sub-operations associated with this operation which generated warning responses.
DATA_ELEM(0000, 1030, AE, "Move Originator Application Entity Title") // Contains the DICOM AE Title of the DICOM AE which invoked the C-MOVE operation from which this C-STORE sub-operation is being performed.
DATA_ELEM(0000, 1031, US, "Move Originator Message ID") // Contains the Message ID (0000,0110) of the C-MOVE-RQ Message from which this C-STORE sub-operations is being performed.

DATA_ELEM(0002, 0001, OB, "File Meta Information Version")
DATA_ELEM(0002, 0002, UI, "Media Storage SOP Class UID")
DATA_ELEM(0002, 0003, UI, "Media Storage SOP Instance UID")
DATA_ELEM(0002, 0010, UI, "Transfer Syntax UID")
DATA_ELEM(0002, 0012, UI, "Implementation Class UID")
DATA_ELEM(0002, 0013, SH, "Implementation Version Name")
DATA_ELEM(0002, 0016, AE, "Source Application Entity Title")
DATA_ELEM(0002, 0100, UI, "Private Information Creator UID")
DATA_ELEM(0002, 0102, OB, "Private Information")

DATA_ELEM(0004, 1130, CS, "File-set ID")
DATA_ELEM(0004, 1141, CS, "File-set Descriptor File ID")
DATA_ELEM(0004, 1142, CS, "Specific Character Set of File-set Descriptor File")
DATA_ELEM(0004, 1200, UL, "Offset of the First Directory Record of the Root Directory Entity")
DATA_ELEM(0004, 1202, UL, "Offset of the Last Directory Record of the Root Directory Entity")
DATA_ELEM(0004, 1212, US, "File-set Consistency Flag")
DATA_ELEM(0004, 1220, SQ, "Directory Record Sequence")
DATA_ELEM(0004, 1400, UL, "Offset of the Next Directory Record")
DATA_ELEM(0004, 1410, US, "Record In-use Flag")
DATA_ELEM(0004, 1420, UL, "Offset of Referenced Lower-Level Directory Entity")
DATA_ELEM(0004, 1430, CS, "Directory Record Type")
DATA_ELEM(0004, 1432, UI, "Private Record UID")
DATA_ELEM(0004, 1500, CS, "Referenced File ID")
DATA_ELEM(0004, 1504, UL, "MRDR Directory Record Offset")
DATA_ELEM(0004, 1510, UI, "Referenced SOP Class UID in File")
DATA_ELEM(0004, 1511, UI, "Referenced SOP Instance UID in File")
DATA_ELEM(0004, 1512, UI, "Referenced Transfer Syntax UID in File")
DATA_ELEM(0004, 1600, UL, "Number of References")

DATA_ELEM(0008, 0005, CS, "Specific Character Set")
DATA_ELEM(0008, 0008, CS, "Image Type")
DATA_ELEM(0008, 0012, DA, "Instance Creation Date")
DATA_ELEM(0008, 0013, TM, "Instance Creation Time")
DATA_ELEM(0008, 0014, UI, "Instance Creator UID")
DATA_ELEM(0008, 0016, UI, "SOP Class UID")
DATA_ELEM(0008, 0018, UI, "SOP Instance UID")
DATA_ELEM(0008, 0020, DA, "Study Date")
DATA_ELEM(0008, 0021, DA, "Series Date")
DATA_ELEM(0008, 0022, DA, "Acquisition Date")
DATA_ELEM(0008, 0023, DA, "Content Date")
DATA_ELEM(0008, 0024, DA, "Overlay Date")
DATA_ELEM(0008, 0025, DA, "Curve Date")
DATA_ELEM(0008, 002A, DT, "Acquisition Datetime")
DATA_ELEM(0008, 0030, TM, "Study Time")
DATA_ELEM(0008, 0031, TM, "Series Time")
DATA_ELEM(0008, 0032, TM, "Acquisition Time")
DATA_ELEM(0008, 0033, TM, "Content Time")
DATA_ELEM(0008, 0034, TM, "Overlay Time")
DATA_ELEM(0008, 0035, TM, "Curve Time")
DATA_ELEM(0008, 0042, CS, "Nuclear Medicine Series Type (RET)")
DATA_ELEM(0008, 0050, SH, "Accession Number")
DATA_ELEM(0008, 0052, CS, "Query/Retrieve Level")
DATA_ELEM(0008, 0054, AE, "Retrieve AE Title")
DATA_ELEM(0008, 0056, CS, "Instance Availability")
DATA_ELEM(0008, 0058, UI, "Failed SOP Instance UID List")
DATA_ELEM(0008, 0060, CS, "Modality")
DATA_ELEM(0008, 0061, CS, "Modalities in Study")
DATA_ELEM(0008, 0062, UI, "SOP Classes in Study")
DATA_ELEM(0008, 0064, CS, "Conversion Type")
DATA_ELEM(0008, 0068, CS, "Presentation Intent Type")
DATA_ELEM(0008, 0070, LO, "Manufacturer")
DATA_ELEM(0008, 0080, LO, "Institution Name")
DATA_ELEM(0008, 0081, ST, "Institution Address")
DATA_ELEM(0008, 0082, SQ, "Institution Code Sequence")
DATA_ELEM(0008, 0090, PN, "Referring Physician's Name")
DATA_ELEM(0008, 0092, ST, "Referring Physician's Address")
DATA_ELEM(0008, 0094, SH, "Referring Physician's Telephone Numbers")
DATA_ELEM(0008, 0096, SQ, "Referring Physician Identification Sequence")
DATA_ELEM(0008, 0100, SH, "Code Value")
DATA_ELEM(0008, 0102, SH, "Coding Scheme Designator")
DATA_ELEM(0008, 0103, SH, "Coding Scheme Version")
DATA_ELEM(0008, 0104, LO, "Code Meaning")
DATA_ELEM(0008, 0105, CS, "Mapping Resource")
DATA_ELEM(0008, 0106, DT, "Context Group Version")
DATA_ELEM(0008, 0107, DT, "Context Group Local Version")
DATA_ELEM(0008, 0110, SQ, "Coding Scheme Identification Sequence")
DATA_ELEM(0008, 0112, LO, "Coding Scheme Registry")
DATA_ELEM(0008, 0114, ST, "Coding Scheme External ID")
DATA_ELEM(0008, 0115, ST, "Coding Scheme Name")
DATA_ELEM(0008, 0116, ST, "Responsible Organization")
DATA_ELEM(0008, 010B, CS, "Code Set Extension Flag")
DATA_ELEM(0008, 010C, UI, "Private Coding Scheme Creator UID")
DATA_ELEM(0008, 010D, UI, "Code Set Extension Creator UID")
DATA_ELEM(0008, 010F, CS, "Context Identifier")
DATA_ELEM(0008, 0201, SH, "Timezone Offset From UTC")
DATA_ELEM(0008, 1010, SH, "Station Name")
DATA_ELEM(0008, 1030, LO, "Study Description")
DATA_ELEM(0008, 1032, SQ, "Procedure Code Sequence")
DATA_ELEM(0008, 103E, LO, "Series Description")
DATA_ELEM(0008, 1040, LO, "Institutional Department Name")
DATA_ELEM(0008, 1048, PN, "Physician(s) of Record")
DATA_ELEM(0008, 1049, SQ, "Physician(s) of Record Identification Sequence")
DATA_ELEM(0008, 1050, PN, "Performing Physician's Name")
DATA_ELEM(0008, 1052, SQ, "Performing Physician Identification Sequence")
DATA_ELEM(0008, 1060, PN, "Name of Physician(s) Reading Study")
DATA_ELEM(0008, 1062, SQ, "Physician(s) Reading Study Identification Sequence")
DATA_ELEM(0008, 1070, PN, "Operators' Name")
DATA_ELEM(0008, 1072, SQ, "Operator Identification Sequence")
DATA_ELEM(0008, 1080, LO, "Admitting Diagnoses Description")
DATA_ELEM(0008, 1084, SQ, "Admitting Diagnosis Code Sequence")
DATA_ELEM(0008, 1090, LO, "Manufacturer's Model Name")
DATA_ELEM(0008, 1100, SQ, "Referenced Results Sequence")
DATA_ELEM(0008, 1110, SQ, "Referenced Study Sequence")
DATA_ELEM(0008, 1111, SQ, "Referenced Study Component Sequence")
DATA_ELEM(0008, 1115, SQ, "Referenced Series Sequence")
DATA_ELEM(0008, 1120, SQ, "Referenced Patient Sequence")
DATA_ELEM(0008, 1125, SQ, "Referenced Visit Sequence")
DATA_ELEM(0008, 1130, SQ, "Referenced Overlay Sequence")
DATA_ELEM(0008, 1140, SQ, "Referenced Image Sequence")
DATA_ELEM(0008, 1145, SQ, "Referenced Curve Sequence")
DATA_ELEM(0008, 114A, SQ, "Referenced Instance Sequence")
DATA_ELEM(0008, 1150, UI, "Referenced SOP Class UID")
DATA_ELEM(0008, 1155, UI, "Referenced SOP Instance UID")
DATA_ELEM(0008, 115A, UI, "SOP Classes Supported")
DATA_ELEM(0008, 1160, IS, "Referenced Frame Number")
DATA_ELEM(0008, 1195, UI, "Transaction UID")
DATA_ELEM(0008, 1197, US, "Failure Reason")
DATA_ELEM(0008, 1198, SQ, "Failed SOP Sequence")
DATA_ELEM(0008, 1199, SQ, "Referenced SOP Sequence")
DATA_ELEM(0008, 2110, CS, "Lossy Image Compression (RET)")
DATA_ELEM(0008, 2111, ST, "Derivation Description")
DATA_ELEM(0008, 2112, SQ, "Source Image Sequence")
DATA_ELEM(0008, 2120, SH, "Stage Name")
DATA_ELEM(0008, 2122, IS, "Stage Number")
DATA_ELEM(0008, 2124, IS, "Number of Stages")
DATA_ELEM(0008, 2128, IS, "View Number")
DATA_ELEM(0008, 2129, IS, "Number of Event Timers")
DATA_ELEM(0008, 212A, IS, "Number of Views in Stage")
DATA_ELEM(0008, 2130, DS, "Event Elapsed Time(s)")
DATA_ELEM(0008, 2132, LO, "Event Timer Name(s)")
DATA_ELEM(0008, 2142, IS, "Start Trim")
DATA_ELEM(0008, 2143, IS, "Stop Trim")
DATA_ELEM(0008, 2144, IS, "Recommended Display Frame Rate")
DATA_ELEM(0008, 2200, CS, "Transducer Position (RET)")
DATA_ELEM(0008, 2204, CS, "Transducer Orientation (RET)")
DATA_ELEM(0008, 2208, CS, "Anatomic Structure (RET)")
DATA_ELEM(0008, 2218, SQ, "Anatomic Region Sequence")
DATA_ELEM(0008, 2220, SQ, "Anatomic Region Modifier Sequence")
DATA_ELEM(0008, 2228, SQ, "Primary Anatomic Structure Sequence")
DATA_ELEM(0008, 2229, SQ, "Anatomic Structure, Space or Region Sequence")
DATA_ELEM(0008, 2230, SQ, "Primary Anatomic Structure Modifier Sequence")
DATA_ELEM(0008, 2240, SQ, "Transducer Position Sequence")
DATA_ELEM(0008, 2242, SQ, "Transducer Position Modifier Sequence")
DATA_ELEM(0008, 2244, SQ, "Transducer Orientation Sequence")
DATA_ELEM(0008, 2246, SQ, "Transducer Orientation Modifier Sequence")
DATA_ELEM(0008, 9123, UI, "Creator-Version UID")

DATA_ELEM(0010, 0010, PN, "Patient's Name")
DATA_ELEM(0010, 0020, LO, "Patient ID")
DATA_ELEM(0010, 0021, LO, "Issuer of Patient ID")
DATA_ELEM(0010, 0030, DA, "Patient's Birth Date")
DATA_ELEM(0010, 0032, TM, "Patient's Birth Time")
DATA_ELEM(0010, 0040, CS, "Patient's Sex")
DATA_ELEM(0010, 0050, SQ, "Patient's Insurance Plan Code Sequence")
DATA_ELEM(0010, 1000, LO, "Other Patient IDs")
DATA_ELEM(0010, 1001, PN, "Other Patient Names")
DATA_ELEM(0010, 1005, PN, "Patient's Birth Name")
DATA_ELEM(0010, 1010, AS, "Patient's Age")
DATA_ELEM(0010, 1020, DS, "Patient's Size")
DATA_ELEM(0010, 1030, DS, "Patient's Weight")
DATA_ELEM(0010, 1040, LO, "Patient's Address")
DATA_ELEM(0010, 1060, PN, "Patient's Mother's Birth Name")
DATA_ELEM(0010, 1080, LO, "Military Rank")
DATA_ELEM(0010, 1081, LO, "Branch of Service")
DATA_ELEM(0010, 1090, LO, "Medical Record Locator")
DATA_ELEM(0010, 2000, LO, "Medical Alerts")
DATA_ELEM(0010, 2110, LO, "Contrast Allergies")
DATA_ELEM(0010, 2150, LO, "Country of Residence")
DATA_ELEM(0010, 2152, LO, "Region of Residence")
DATA_ELEM(0010, 2154, SH, "Patient's Telephone Numbers")
DATA_ELEM(0010, 2160, SH, "Ethnic Group")
DATA_ELEM(0010, 2180, SH, "Occupation")
DATA_ELEM(0010, 21A0, CS, "Smoking Status")
DATA_ELEM(0010, 21B0, LT, "Additional Patient History")
DATA_ELEM(0010, 21C0, US, "Pregnancy Status")
DATA_ELEM(0010, 21D0, DA, "Last Menstrual Date")
DATA_ELEM(0010, 21F0, LO, "Patient's Religious Preference")
DATA_ELEM(0010, 4000, LT, "Patient Comments")

DATA_ELEM(0012, 0010, LO, "Clinical Trial Sponsor Name")
DATA_ELEM(0012, 0020, LO, "Clinical Trial Protocol ID")
DATA_ELEM(0012, 0021, LO, "Clinical Trial Protocol Name")
DATA_ELEM(0012, 0030, LO, "Clinical Trial Site ID")
DATA_ELEM(0012, 0031, LO, "Clinical Trial Site Name")
DATA_ELEM(0012, 0040, LO, "Clinical Trial Subject ID")
DATA_ELEM(0012, 0042, LO, "Clinical Trial Subject Reading ID")
DATA_ELEM(0012, 0050, LO, "Clinical Trial Time Point ID")
DATA_ELEM(0012, 0051, ST, "Clinical Trial Time Point Description")
DATA_ELEM(0012, 0060, LO, "Clinical Trial Coordinating Center Name")

DATA_ELEM(0018, 0010, LO, "Contrast/Bolus Agent")
DATA_ELEM(0018, 0012, SQ, "Contrast/Bolus Agent Sequence")
DATA_ELEM(0018, 0014, SQ, "Contrast/Bolus Administration Route Sequence")
DATA_ELEM(0018, 0015, CS, "Body Part Examined")
DATA_ELEM(0018, 0020, CS, "Scanning Sequence")
DATA_ELEM(0018, 0021, CS, "Sequence Variant")
DATA_ELEM(0018, 0022, CS, "Scan Options")
DATA_ELEM(0018, 0023, CS, "MR Acquisition Type")
DATA_ELEM(0018, 0024, SH, "Sequence Name")
DATA_ELEM(0018, 0025, CS, "Angio Flag")
DATA_ELEM(0018, 0026, SQ, "Intervention Drug Information Sequence")
DATA_ELEM(0018, 0027, TM, "Intervention Drug Stop Time")
DATA_ELEM(0018, 0028, DS, "Intervention Drug Dose")
DATA_ELEM(0018, 0029, SQ, "Intervention Drug Code Sequence")
DATA_ELEM(0018, 002A, SQ, "Additional Drug Sequence")
DATA_ELEM(0018, 0030, LO, "Radionuclide (RET)")
DATA_ELEM(0018, 0031, LO, "Radiopharmaceutical")
DATA_ELEM(0018, 0032, DS, "Energy Window Centerline (RET)")
DATA_ELEM(0018, 0033, DS, "Energy Window Total Width (RET)")
DATA_ELEM(0018, 0034, LO, "Intervention Drug Name")
DATA_ELEM(0018, 0035, TM, "Intervention Drug Start Time")
DATA_ELEM(0018, 0036, SQ, "Interventional Therapy Sequence")
DATA_ELEM(0018, 0037, CS, "Therapy Type")
DATA_ELEM(0018, 0038, CS, "Interventional Status")
DATA_ELEM(0018, 0039, CS, "Therapy Description")
DATA_ELEM(0018, 0040, IS, "Cine Rate")
DATA_ELEM(0018, 0050, DS, "Slice Thickness")
DATA_ELEM(0018, 0060, DS, "KVP")
DATA_ELEM(0018, 0070, IS, "Counts Accumulated")
DATA_ELEM(0018, 0071, CS, "Acquisition Termination Condition")
DATA_ELEM(0018, 0072, DS, "Effective Series Duration")
DATA_ELEM(0018, 0073, CS, "Acquisition Start Condition")
DATA_ELEM(0018, 0074, IS, "Acquisition Start Condition Data")
DATA_ELEM(0018, 0075, IS, "Acquisition Termination Condition Data")
DATA_ELEM(0018, 0080, DS, "Repetition Time")
DATA_ELEM(0018, 0081, DS, "Echo Time")
DATA_ELEM(0018, 0082, DS, "Inversion Time")
DATA_ELEM(0018, 0083, DS, "Number of Averages")
DATA_ELEM(0018, 0084, DS, "Imaging Frequency")
DATA_ELEM(0018, 0085, SH, "Imaged Nucleus")
DATA_ELEM(0018, 0086, IS, "Echo Number(s)")
DATA_ELEM(0018, 0087, DS, "Magnetic Field Strength")
DATA_ELEM(0018, 0088, DS, "Spacing Between Slices")
DATA_ELEM(0018, 0089, IS, "Number of Phase Encoding Steps")
DATA_ELEM(0018, 0090, DS, "Data Collection Diameter")
DATA_ELEM(0018, 0091, IS, "Echo Train Length")
DATA_ELEM(0018, 0093, DS, "Percent Sampling")
DATA_ELEM(0018, 0094, DS, "Percent Phase Field of View")
DATA_ELEM(0018, 0095, DS, "Pixel Bandwidth")
DATA_ELEM(0018, 1000, LO, "Device Serial Number")
DATA_ELEM(0018, 1004, LO, "Plate ID")
DATA_ELEM(0018, 1010, LO, "Secondary Capture Device ID")
DATA_ELEM(0018, 1011, LO, "Hardcopy Creation Device ID")
DATA_ELEM(0018, 1012, DA, "Date of Secondary Capture")
DATA_ELEM(0018, 1014, TM, "Time of Secondary Capture")
DATA_ELEM(0018, 1016, LO, "Secondary Capture Device Manufacturer")
DATA_ELEM(0018, 1017, LO, "Hardcopy Device Manufacturer")
DATA_ELEM(0018, 1018, LO, "Secondary Capture Device Manufacturer's Model Name")
DATA_ELEM(0018, 1019, LO, "Secondary Capture Device Software Version(s)")
DATA_ELEM(0018, 101A, LO, "Hardcopy Device Software Version")
DATA_ELEM(0018, 101B, LO, "Hardcopy Device Manfuacturer's Model Name")
DATA_ELEM(0018, 1020, LO, "Software Version(s)")
DATA_ELEM(0018, 1022, SH, "Video Image Format Acquired")
DATA_ELEM(0018, 1023, LO, "Digital Image Format Acquired")
DATA_ELEM(0018, 1030, LO, "Protocol Name")
DATA_ELEM(0018, 1040, LO, "Contrast/Bolus Route")
DATA_ELEM(0018, 1041, DS, "Contrast/Bolus Volume")
DATA_ELEM(0018, 1042, TM, "Contrast/Bolus Start Time")
DATA_ELEM(0018, 1043, TM, "Contrast/Bolus Stop Time")
DATA_ELEM(0018, 1044, DS, "Contrast/Bolus Total Dose")
DATA_ELEM(0018, 1045, IS, "Syringe Counts")
DATA_ELEM(0018, 1046, DS, "Contrast Flow Rate(s)")
DATA_ELEM(0018, 1047, DS, "Contrast Flow Duration(s)")
DATA_ELEM(0018, 1048, CS, "Contrast/Bolus Ingredient")
DATA_ELEM(0018, 1049, DS, "Contrast/Bolus Ingredient Concentration")
DATA_ELEM(0018, 1050, DS, "Spatial Resolution")
DATA_ELEM(0018, 1060, DS, "Trigger Time")
DATA_ELEM(0018, 1061, LO, "Trigger Source or Type")
DATA_ELEM(0018, 1062, IS, "Nominal Interval")
DATA_ELEM(0018, 1063, DS, "Frame Time")
DATA_ELEM(0018, 1064, LO, "Framing Type")
DATA_ELEM(0018, 1065, DS, "Frame Time Vector")
DATA_ELEM(0018, 1066, DS, "Frame Delay")
DATA_ELEM(0018, 1067, DS, "Image Trigger Delay")
DATA_ELEM(0018, 1068, DS, "Multiplex Group Time Offset")
DATA_ELEM(0018, 1069, DS, "Trigger Time Offset")
DATA_ELEM(0018, 106A, CS, "Synchronization Trigger")
DATA_ELEM(0018, 106C, US, "Synchronization Channel")
DATA_ELEM(0018, 106E, UL, "Trigger Sample Position")
DATA_ELEM(0018, 1070, LO, "Radiopharmaceutical Route")
DATA_ELEM(0018, 1071, DS, "Radiopharmaceutical Volume")
DATA_ELEM(0018, 1072, TM, "Radiopharmaceutical Start Time")
DATA_ELEM(0018, 1073, TM, "Radiopharmaceutical Stop Time")
DATA_ELEM(0018, 1074, DS, "Radionuclide Total Dose")
DATA_ELEM(0018, 1075, DS, "Radionuclide Half Life")
DATA_ELEM(0018, 1076, DS, "Radionuclide Positron Fraction")
DATA_ELEM(0018, 1077, DS, "Radiopharmaceutical Specific Activity")
DATA_ELEM(0018, 1080, CS, "Beat Rejection Flag")
DATA_ELEM(0018, 1081, IS, "Low R-R Value")
DATA_ELEM(0018, 1082, IS, "High R-R Value")
DATA_ELEM(0018, 1083, IS, "Intervals Acquired")
DATA_ELEM(0018, 1084, IS, "Intervals Rejected")
DATA_ELEM(0018, 1085, LO, "PVC Rejection")
DATA_ELEM(0018, 1086, IS, "Skip Beats")
DATA_ELEM(0018, 1088, IS, "Heart Rate")
DATA_ELEM(0018, 1090, IS, "Cardiac Number of Images")
DATA_ELEM(0018, 1094, IS, "Trigger Window")
DATA_ELEM(0018, 1100, DS, "Reconstruction Diameter")
DATA_ELEM(0018, 1110, DS, "Distance Source to Detector")
DATA_ELEM(0018, 1111, DS, "Distance Source to Patient")
DATA_ELEM(0018, 1114, DS, "Estimated Radiographic Magnification Factor")
DATA_ELEM(0018, 1120, DS, "Gantry/Detector Tilt")
DATA_ELEM(0018, 1121, DS, "Gantry/Detector Slew")
DATA_ELEM(0018, 1130, DS, "Table Height")
DATA_ELEM(0018, 1131, DS, "Table Traverse")
DATA_ELEM(0018, 1134, CS, "Table Motion")
DATA_ELEM(0018, 1135, DS, "Table Vertical Increment")
DATA_ELEM(0018, 1136, DS, "Table Lateral Increment")
DATA_ELEM(0018, 1137, DS, "Table Longitudinal Increment")
DATA_ELEM(0018, 1138, DS, "Table Angle")
DATA_ELEM(0018, 113A, CS, "Table Type")
DATA_ELEM(0018, 1140, CS, "Rotation Direction")
DATA_ELEM(0018, 1141, DS, "Angular Position")
DATA_ELEM(0018, 1142, DS, "Radial Position")
DATA_ELEM(0018, 1143, DS, "Scan Arc")
DATA_ELEM(0018, 1144, DS, "Angular Step")
DATA_ELEM(0018, 1145, DS, "Center of Rotation Offset")
DATA_ELEM(0018, 1146, DS, "Rotation Offset (RET)")
DATA_ELEM(0018, 1147, CS, "Field of View Shape")
DATA_ELEM(0018, 1149, IS, "Field of View Dimension(s)")
DATA_ELEM(0018, 1150, IS, "Exposure Time")
DATA_ELEM(0018, 1151, IS, "X-ray Tube Current")
DATA_ELEM(0018, 1152, IS, "Exposure")
DATA_ELEM(0018, 1153, IS, "Exposure in uAs")
DATA_ELEM(0018, 1154, DS, "Average Pulse Width")
DATA_ELEM(0018, 1155, CS, "Radiation Setting")
DATA_ELEM(0018, 1156, CS, "Rectification Type")
DATA_ELEM(0018, 115A, CS, "Radiation Mode")
DATA_ELEM(0018, 115E, DS, "Image Area Dose Product")
DATA_ELEM(0018, 1160, SH, "Filter Type")
DATA_ELEM(0018, 1161, LO, "Type of Filters")
DATA_ELEM(0018, 1162, DS, "Intensifier Size")
DATA_ELEM(0018, 1164, DS, "Imager Pixel Spacing")
DATA_ELEM(0018, 1166, CS, "Grid")
DATA_ELEM(0018, 1170, IS, "Generator Power")
DATA_ELEM(0018, 1180, SH, "Collimator/grid Name")
DATA_ELEM(0018, 1181, CS, "Collimator Type")
DATA_ELEM(0018, 1182, IS, "Focal Distance")
DATA_ELEM(0018, 1183, DS, "X Focus Center")
DATA_ELEM(0018, 1184, DS, "Y Focus Center")
DATA_ELEM(0018, 1190, DS, "Focal Spot(s)")
DATA_ELEM(0018, 1191, CS, "Anode Target Material")
DATA_ELEM(0018, 11A0, DS, "Body Part Thickness")
DATA_ELEM(0018, 11A2, DS, "Compression Force")
DATA_ELEM(0018, 1200, DA, "Date of Last Calibration")
DATA_ELEM(0018, 1201, TM, "Time of Last Calibration")
DATA_ELEM(0018, 1210, SH, "Convolution Kernel")
DATA_ELEM(0018, 1242, IS, "Actual Frame Duration")
DATA_ELEM(0018, 1243, IS, "Count Rate")
DATA_ELEM(0018, 1244, US, "Preferred Playback Sequencing")
DATA_ELEM(0018, 1250, SH, "Receiving Coil")
DATA_ELEM(0018, 1251, SH, "Transmitting Coil")
DATA_ELEM(0018, 1260, SH, "Plate Type")
DATA_ELEM(0018, 1261, LO, "Phosphor Type")
DATA_ELEM(0018, 1300, DS, "Scan Velocity")
DATA_ELEM(0018, 1301, CS, "Whole Body Technique")
DATA_ELEM(0018, 1302, IS, "Scan Length")
DATA_ELEM(0018, 1310, US, "Acquisition Matrix")
DATA_ELEM(0018, 1312, CS, "Phase Encoding Direction")
DATA_ELEM(0018, 1314, DS, "Flip Angle")
DATA_ELEM(0018, 1315, CS, "Variable Flip Angle Flag")
DATA_ELEM(0018, 1316, DS, "SAR")
DATA_ELEM(0018, 1318, DS, "dB/dt")
DATA_ELEM(0018, 1400, LO, "Acquisition Device Processing Description")
DATA_ELEM(0018, 1401, LO, "Acquisition Device Processing Code")
DATA_ELEM(0018, 1402, CS, "Cassette Orientation")
DATA_ELEM(0018, 1403, CS, "Cassette Size")
DATA_ELEM(0018, 1404, US, "Exposures on Plate")
DATA_ELEM(0018, 1405, IS, "Relative X-ray Exposure")
DATA_ELEM(0018, 1450, CS, "Column Angulation")
DATA_ELEM(0018, 1460, DS, "Tomo Layer Height")
DATA_ELEM(0018, 1470, DS, "Tomo Angle")
DATA_ELEM(0018, 1480, DS, "Tomo Time")
DATA_ELEM(0018, 1490, CS, "Tomo Type")
DATA_ELEM(0018, 1491, CS, "Tomo Class")
DATA_ELEM(0018, 1495, IS, "Number of Tomosynthesis Source Images")
DATA_ELEM(0018, 1500, CS, "Positioner Motion")
DATA_ELEM(0018, 1508, CS, "Positioner Type")
DATA_ELEM(0018, 1510, DS, "Positioner Primary Angle")
DATA_ELEM(0018, 1511, DS, "Positioner Secondary Angle")
DATA_ELEM(0018, 1520, DS, "Positioner Primary Angle Increment")
DATA_ELEM(0018, 1521, DS, "Positioner Secondary Angle Increment")
DATA_ELEM(0018, 1530, DS, "Detector Primary Angle")
DATA_ELEM(0018, 1531, DS, "Detector Secondary Angle")
DATA_ELEM(0018, 1600, CS, "Shutter Shape")
DATA_ELEM(0018, 1602, IS, "Shutter Left Vertical Edge")
DATA_ELEM(0018, 1604, IS, "Shutter Right Vertical Edge")
DATA_ELEM(0018, 1606, IS, "Shutter Upper Horizontal Edge")
DATA_ELEM(0018, 1608, IS, "Shutter Lower Horizontal Edge")
DATA_ELEM(0018, 1610, IS, "Center of Circular Shutter")
DATA_ELEM(0018, 1612, IS, "Radius of Circular Shutter")
DATA_ELEM(0018, 1620, IS, "Vertices of the Polygonal Shutter")
DATA_ELEM(0018, 1622, US, "Shutter Presentation Value")
DATA_ELEM(0018, 1623, US, "Shutter Overlay Group")
DATA_ELEM(0018, 1700, CS, "Collimator Shape")
DATA_ELEM(0018, 1702, IS, "Collimator Left Vertical Edge")
DATA_ELEM(0018, 1704, IS, "Collimator Right Vertical Edge")
DATA_ELEM(0018, 1706, IS, "Collimator Upper Horizontal Edge")
DATA_ELEM(0018, 1708, IS, "Collimator Lower Horizontal Edge")
DATA_ELEM(0018, 1710, IS, "Center of Circular Collimator")
DATA_ELEM(0018, 1712, IS, "Radius of Circular Collimator")
DATA_ELEM(0018, 1720, IS, "Vertices of the Polygonal Collimator")
DATA_ELEM(0018, 1800, CS, "Acquisition Time Synchronized")
DATA_ELEM(0018, 1802, CS, "Time Distribution Protocol")
DATA_ELEM(0018, 1801, SH, "Time Source")
DATA_ELEM(0018, 2001, IS, "Page Number Vector")
DATA_ELEM(0018, 2002, SH, "Frame Label Vector")
DATA_ELEM(0018, 2003, DS, "Frame Primary Angle Vector")
DATA_ELEM(0018, 2004, DS, "Frame Secondary Angle Vector")
DATA_ELEM(0018, 2005, DS, "Slice Location Vector")
DATA_ELEM(0018, 2006, SH, "Display Window Label Vector")
DATA_ELEM(0018, 2010, DS, "Nominal Scanned Pixel Spacing")
DATA_ELEM(0018, 2020, CS, "Digitizing Device Transport Direction")
DATA_ELEM(0018, 2030, DS, "Rotation of Scanned Film")
DATA_ELEM(0018, 5000, SH, "Output Power")
DATA_ELEM(0018, 5010, LO, "Transducer Data")
DATA_ELEM(0018, 5012, DS, "Focus Depth")
DATA_ELEM(0018, 5020, LO, "Processing Function")
DATA_ELEM(0018, 5021, LO, "Postprocessing Function")
DATA_ELEM(0018, 5022, DS, "Mechanical Index")
DATA_ELEM(0018, 5024, DS, "Thermal Index")
DATA_ELEM(0018, 5026, DS, "Cranial Thermal Index")
DATA_ELEM(0018, 5027, DS, "Soft Tissue Thermal Index")
DATA_ELEM(0018, 5028, DS, "Soft Tissue-focus Thermal Index")
DATA_ELEM(0018, 5029, DS, "Soft Tissue-surface Thermal Index")
DATA_ELEM(0018, 5050, IS, "Depth of Scan Field")
DATA_ELEM(0018, 5100, CS, "Patient Position")
DATA_ELEM(0018, 5101, CS, "View Position")
DATA_ELEM(0018, 5104, SQ, "Projection Eponymous Name Code Sequence")
DATA_ELEM(0018, 5210, DS, "Image Transformation Matrix")
DATA_ELEM(0018, 5212, DS, "Image Translation Vector")
DATA_ELEM(0018, 6000, DS, "Sensitivity")
DATA_ELEM(0018, 6011, SQ, "Sequence of Ultrasound Regions")
DATA_ELEM(0018, 6012, US, "Region Spatial Format")
DATA_ELEM(0018, 6014, US, "Region Data Type")
DATA_ELEM(0018, 6016, UL, "Region Flags")
DATA_ELEM(0018, 6018, UL, "Region Location Min X 0")
DATA_ELEM(0018, 601A, UL, "Region Location Min Y 0")
DATA_ELEM(0018, 601C, UL, "Region Location Max X 1")
DATA_ELEM(0018, 601E, UL, "Region Location Max Y 1")
DATA_ELEM(0018, 6020, SL, "Reference Pixel X 0")
DATA_ELEM(0018, 6022, SL, "Reference Pixel Y 0")
DATA_ELEM(0018, 6024, US, "Physical Units X Direction")
DATA_ELEM(0018, 6026, US, "Physical Units Y Direction")
DATA_ELEM(0018, 6028, FD, "Reference Pixel Physical Value X")
DATA_ELEM(0018, 602A, FD, "Reference Pixel Physical Value Y")
DATA_ELEM(0018, 602C, FD, "Physical Delta X")
DATA_ELEM(0018, 602E, FD, "Physical Delta Y")
DATA_ELEM(0018, 6030, UL, "Transducer Frequency")
DATA_ELEM(0018, 6031, CS, "Transducer Type")
DATA_ELEM(0018, 6032, UL, "Pulse Repetition Frequency")
DATA_ELEM(0018, 6034, FD, "Doppler Correction Angle")
DATA_ELEM(0018, 6036, FD, "Steering Angle")
DATA_ELEM(0018, 6038, UL, "Doppler Sample Volume X Position")
DATA_ELEM(0018, 603A, UL, "Doppler Sample Volume Y Position")
DATA_ELEM(0018, 603C, UL, "TM-Line Position X 0")
DATA_ELEM(0018, 603E, UL, "TM-Line Position Y 0")
DATA_ELEM(0018, 6040, UL, "TM-Line Position X 1")
DATA_ELEM(0018, 6042, UL, "TM-Line Position Y 1")
DATA_ELEM(0018, 6044, US, "Pixel Component Organization")
DATA_ELEM(0018, 6046, UL, "Pixel Component Mask")
DATA_ELEM(0018, 6048, UL, "Pixel Component Range Start")
DATA_ELEM(0018, 604A, UL, "Pixel Component Range Stop")
DATA_ELEM(0018, 604C, US, "Pixel Component Physical Units")
DATA_ELEM(0018, 604E, US, "Pixel Component Data Type")
DATA_ELEM(0018, 6050, UL, "Number of Table Break Points")
DATA_ELEM(0018, 6052, UL, "Table of X Break Points")
DATA_ELEM(0018, 6054, FD, "Table of Y Break Points")
DATA_ELEM(0018, 6056, UL, "Number of Table Entries")
DATA_ELEM(0018, 6058, UL, "Table of Pixel Values")
DATA_ELEM(0018, 605A, FL, "Table of Parameter Values")
DATA_ELEM(0018, 7000, CS, "Detector Conditions Nominal Flag")
DATA_ELEM(0018, 7001, DS, "Detector Temperature")
DATA_ELEM(0018, 7004, CS, "Detector Type")
DATA_ELEM(0018, 7005, CS, "Detector Configuration")
DATA_ELEM(0018, 7006, LT, "Detector Description")
DATA_ELEM(0018, 7008, LT, "Detector Mode")
DATA_ELEM(0018, 700A, SH, "Detector ID")
DATA_ELEM(0018, 700C, DA, "Date of Last Detector Calibration")
DATA_ELEM(0018, 700E, TM, "Time of Last Detector Calibration")
DATA_ELEM(0018, 7010, IS, "Exposures on Detector Since Last Calibration")
DATA_ELEM(0018, 7011, IS, "Exposures on Detector Since Manufactured")
DATA_ELEM(0018, 7012, DS, "Detector Time Since Last Exposure")
DATA_ELEM(0018, 7014, DS, "Detector Active Time")
DATA_ELEM(0018, 7016, DS, "Detector Activation Offset From Exposure")
DATA_ELEM(0018, 701A, DS, "Detector Binning")
DATA_ELEM(0018, 7020, DS, "Detector Element Physical Size")
DATA_ELEM(0018, 7022, DS, "Detector Element Spacing")
DATA_ELEM(0018, 7024, CS, "Detector Active Shape")
DATA_ELEM(0018, 7026, DS, "Detector Active Dimension(s)")
DATA_ELEM(0018, 7028, DS, "Detector Active Origin")
DATA_ELEM(0018, 7030, DS, "Field of View Origin")
DATA_ELEM(0018, 7032, DS, "Field of View Rotation")
DATA_ELEM(0018, 7034, CS, "Field of View Horizontal Flip")
DATA_ELEM(0018, 7040, LT, "Grid Absorbing Material")
DATA_ELEM(0018, 7041, LT, "Grid Spacing Material")
DATA_ELEM(0018, 7042, DS, "Grid Thickness")
DATA_ELEM(0018, 7044, DS, "Grid Pitch")
DATA_ELEM(0018, 7046, IS, "Grid Aspect Ratio")
DATA_ELEM(0018, 7048, DS, "Grid Period")
DATA_ELEM(0018, 704C, DS, "Grid Focal Distance")
DATA_ELEM(0018, 7050, CS, "Filter Material")
DATA_ELEM(0018, 7052, DS, "Filter Thickness Minimum")
DATA_ELEM(0018, 7054, DS, "Filter Thickness Maximum")
DATA_ELEM(0018, 7060, CS, "Exposure Control Mode")
DATA_ELEM(0018, 7062, LT, "Exposure Control Mode Description")
DATA_ELEM(0018, 7064, CS, "Exposure Status")
DATA_ELEM(0018, 7065, DS, "Phototimer Setting")
DATA_ELEM(0018, 8150, DS, "Exposure Time in mS")
DATA_ELEM(0018, 8151, DS, "X-Ray Tube Current in mA")
DATA_ELEM(0018, A001, SQ, "Contributing Equipment Sequence")
DATA_ELEM(0018, A002, DT, "Contribution DateTime")
DATA_ELEM(0018, A003, ST, "Contribution Description")

DATA_ELEM(0020, 000D, UI, "Study Instance UID")
DATA_ELEM(0020, 000E, UI, "Series Instance UID")
DATA_ELEM(0020, 0010, SH, "Study ID")
DATA_ELEM(0020, 0011, IS, "Series Number")
DATA_ELEM(0020, 0012, IS, "Acquisition Number")
DATA_ELEM(0020, 0013, IS, "Instance Number")
DATA_ELEM(0020, 0014, IS, "Isotope Number (RET)")
DATA_ELEM(0020, 0015, IS, "Phase Number (RET)")
DATA_ELEM(0020, 0016, IS, "Interval Number (RET)")
DATA_ELEM(0020, 0017, IS, "Time Slot Number (RET)")
DATA_ELEM(0020, 0018, IS, "Angle Number (RET)")
DATA_ELEM(0020, 0019, IS, "Item Number")
DATA_ELEM(0020, 0020, CS, "Patient Orientation")
DATA_ELEM(0020, 0022, IS, "Overlay Number")
DATA_ELEM(0020, 0024, IS, "Curve Number")
DATA_ELEM(0020, 0026, IS, "Lookup Table Number")
DATA_ELEM(0020, 0032, DS, "Image Position (Patient)")
DATA_ELEM(0020, 0037, DS, "Image Orientation (Patient)")
DATA_ELEM(0020, 0052, UI, "Frame of Reference UID")
DATA_ELEM(0020, 0060, CS, "Laterality")
DATA_ELEM(0020, 0062, CS, "Image Laterality")
DATA_ELEM(0020, 0100, IS, "Temporal Position Identifier")
DATA_ELEM(0020, 0105, IS, "Number of Temporal Positions")
DATA_ELEM(0020, 0110, DS, "Temporal Resolution")
DATA_ELEM(0020, 0200, UI, "Synchronization Frame of Reference UID")
DATA_ELEM(0020, 1000, IS, "Series in Study")
DATA_ELEM(0020, 1002, IS, "Images in Acquisition")
DATA_ELEM(0020, 1004, IS, "Acquisitions in Study")
DATA_ELEM(0020, 1040, LO, "Position Reference Indicator")
DATA_ELEM(0020, 1041, DS, "Slice Location")
DATA_ELEM(0020, 1070, IS, "Other Study Numbers")
DATA_ELEM(0020, 1200, IS, "Number of Patient Related Studies")
DATA_ELEM(0020, 1202, IS, "Number of Patient Related Series")
DATA_ELEM(0020, 1204, IS, "Number of Patient Related Instances")
DATA_ELEM(0020, 1206, IS, "Number of Study Related Series")
DATA_ELEM(0020, 1208, IS, "Number of Study Related Instances")
DATA_ELEM(0020, 1209, IS, "Number of Series Related Instances")
DATA_ELEM(0020, 4000, LT, "Image Comments")

DATA_ELEM(0028, 0002, US, "Samples per Pixel")
DATA_ELEM(0028, 0004, CS, "Photometric Interpretation")
DATA_ELEM(0028, 0006, US, "Planar Configuration")
DATA_ELEM(0028, 0008, IS, "Number of Frames")
DATA_ELEM(0028, 0009, AT, "Frame Increment Pointer")
DATA_ELEM(0028, 0010, US, "Rows")
DATA_ELEM(0028, 0011, US, "Columns")
DATA_ELEM(0028, 0012, US, "Planes")
DATA_ELEM(0028, 0014, US, "Ultrasound Color Data Present")
DATA_ELEM(0028, 0030, DS, "Pixel Spacing")
DATA_ELEM(0028, 0031, DS, "Zoom Factor")
DATA_ELEM(0028, 0032, DS, "Zoom Center")
DATA_ELEM(0028, 0034, IS, "Pixel Aspect Ratio")
DATA_ELEM(0028, 0051, CS, "Corrected Image")
DATA_ELEM(0028, 0100, US, "Bits Allocated")
DATA_ELEM(0028, 0101, US, "Bits Stored")
DATA_ELEM(0028, 0102, US, "High Bit")
DATA_ELEM(0028, 0103, US, "Pixel Representation")
DATA_ELEM(0028, 0106, XS, "Smallest Image Pixel Value")
DATA_ELEM(0028, 0107, XS, "Largest Image Pixel Value")
DATA_ELEM(0028, 0108, XS, "Smallest Pixel Value in Series")
DATA_ELEM(0028, 0109, XS, "Largest Pixel Value in Series")
DATA_ELEM(0028, 0110, XS, "Smallest Image Pixel Value in Plane")
DATA_ELEM(0028, 0111, XS, "Largest Image Pixel Value in Plane")
DATA_ELEM(0028, 0120, XS, "Pixel Padding Value")
DATA_ELEM(0028, 0300, CS, "Quality Control Image")
DATA_ELEM(0028, 0301, CS, "Burned In Annotation")
DATA_ELEM(0028, 1040, CS, "Pixel Intensity Relationship")
DATA_ELEM(0028, 1041, SS, "Pixel Intensity Relationship Sign")
DATA_ELEM(0028, 1050, DS, "Window Center")
DATA_ELEM(0028, 1051, DS, "Window Width")
DATA_ELEM(0028, 1052, DS, "Rescale Intercept")
DATA_ELEM(0028, 1053, DS, "Rescale Slope")
DATA_ELEM(0028, 1054, LO, "Rescale Type")
DATA_ELEM(0028, 1055, LO, "Window Center & Width Explanation")
DATA_ELEM(0028, 1090, CS, "Recommended Viewing Mode")
DATA_ELEM(0028, 1101, XS, "Red Palette Color Lookup Table Descriptor")
DATA_ELEM(0028, 1102, XS, "Green Palette Color Lookup Table Descriptor")
DATA_ELEM(0028, 1103, XS, "Blue Palette Color Lookup Table Descriptor")
DATA_ELEM(0028, 1199, UI, "Palette Color Lookup Table UID")
DATA_ELEM(0028, 1201, OW, "Red Palette Color Lookup Table Data")
DATA_ELEM(0028, 1202, OW, "Green Palette Color Lookup Table Data")
DATA_ELEM(0028, 1203, OW, "Blue Palette Color Lookup Table Data")
DATA_ELEM(0028, 1221, OW, "Segmented Red Palette Color Lookup Table Data")
DATA_ELEM(0028, 1222, OW, "Segmented Green Palette Color Lookup Table Data")
DATA_ELEM(0028, 1223, OW, "Segmented Blue Palette Color Lookup Table Data")
DATA_ELEM(0028, 1300, CS, "Implant Present")
DATA_ELEM(0028, 1350, CS, "Partial View")
DATA_ELEM(0028, 1351, ST, "Partial View Description")
DATA_ELEM(0028, 2110, CS, "Lossy Image Compression")
DATA_ELEM(0028, 2112, DS, "Lossy Image Compression Ratio")
DATA_ELEM(0028, 3000, SQ, "Modality LUT Sequence")
DATA_ELEM(0028, 3002, XS, "LUT Descriptor")
DATA_ELEM(0028, 3003, LO, "LUT Explanation")
DATA_ELEM(0028, 3004, LO, "Modality LUT Type")
DATA_ELEM(0028, 3006, US, "LUT Data")
DATA_ELEM(0028, 3010, SQ, "VOI LUT Sequence")
DATA_ELEM(0028, 3110, SQ, "Softcopy VOI LUT Sequence")
DATA_ELEM(0028, 5000, SQ, "Bi-Plane Acquisition Sequence")
DATA_ELEM(0028, 6010, US, "Representative Frame Number")
DATA_ELEM(0028, 6020, US, "Frame Numbers of Interest (FOI)")
DATA_ELEM(0028, 6022, LO, "Frame(s) of Interest Description")
DATA_ELEM(0028, 6030, US, "Mask Pointer(s)")
DATA_ELEM(0028, 6040, US, "R Wave Pointer")
DATA_ELEM(0028, 6100, SQ, "Mask Subtraction Sequence")
DATA_ELEM(0028, 6101, CS, "Mask Operation")
DATA_ELEM(0028, 6102, US, "Applicable Frame Range")
DATA_ELEM(0028, 6110, US, "Mask Frame Numbers")
DATA_ELEM(0028, 6112, US, "Contrast Frame Averaging")
DATA_ELEM(0028, 6114, FL, "Mask Sub-pixel Shift")
DATA_ELEM(0028, 6120, SS, "TID Offset")
DATA_ELEM(0028, 6190, ST, "Mask Operation Explanation")

DATA_ELEM(0032, 000A, CS, "Study Status ID")
DATA_ELEM(0032, 000C, CS, "Study Priority ID")
DATA_ELEM(0032, 0012, LO, "Study ID Issuer")
DATA_ELEM(0032, 0032, DA, "Study Verified Date")
DATA_ELEM(0032, 0033, TM, "Study Verified Time")
DATA_ELEM(0032, 0034, DA, "Study Read Date")
DATA_ELEM(0032, 0035, TM, "Study Read Time")
DATA_ELEM(0032, 1000, DA, "Scheduled Study Start Date")
DATA_ELEM(0032, 1001, TM, "Scheduled Study Start Time")
DATA_ELEM(0032, 1010, DA, "Scheduled Study Stop Date")
DATA_ELEM(0032, 1011, TM, "Scheduled Study Stop Time")
DATA_ELEM(0032, 1020, LO, "Scheduled Study Location")
DATA_ELEM(0032, 1021, AE, "Scheduled Study Location AE Title(s)")
DATA_ELEM(0032, 1030, LO, "Reason for Study")
DATA_ELEM(0032, 1032, PN, "Requesting Physician")
DATA_ELEM(0032, 1033, LO, "Requesting Service")
DATA_ELEM(0032, 1040, DA, "Study Arrival Date")
DATA_ELEM(0032, 1041, TM, "Study Arrival Time")
DATA_ELEM(0032, 1050, DA, "Study Completion Date")
DATA_ELEM(0032, 1051, TM, "Study Completion Time")
DATA_ELEM(0032, 1055, CS, "Study Component Status ID")
DATA_ELEM(0032, 1060, LO, "Requested Procedure Description")
DATA_ELEM(0032, 1064, SQ, "Requested Procedure Code Sequence")
DATA_ELEM(0032, 1070, LO, "Requested Contrast Agent")
DATA_ELEM(0032, 4000, LT, "Study Comments")

DATA_ELEM(0038, 0004, SQ, "Referenced Patient Alias Sequence")
DATA_ELEM(0038, 0008, CS, "Visit Status ID")
DATA_ELEM(0038, 0010, LO, "Admission ID")
DATA_ELEM(0038, 0011, LO, "Issuer of Admission ID")
DATA_ELEM(0038, 0016, LO, "Route of Admissions")
DATA_ELEM(0038, 001A, DA, "Scheduled Admission Date")
DATA_ELEM(0038, 001B, TM, "Scheduled Admission Time")
DATA_ELEM(0038, 001C, DA, "Scheduled Discharge Date")
DATA_ELEM(0038, 001D, TM, "Scheduled Discharge Time")
DATA_ELEM(0038, 001E, LO, "Scheduled Patient Institution Residence")
DATA_ELEM(0038, 0020, DA, "Admitting Date")
DATA_ELEM(0038, 0021, TM, "Admitting Time")
DATA_ELEM(0038, 0030, DA, "Discharge Date")
DATA_ELEM(0038, 0032, TM, "Discharge Time")
DATA_ELEM(0038, 0040, LO, "Discharge Diagnosis Description")
DATA_ELEM(0038, 0044, SQ, "Discharge Diagnosis Code Sequence")
DATA_ELEM(0038, 0050, LO, "Special Needs")
DATA_ELEM(0038, 0300, LO, "Current Patient Location")
DATA_ELEM(0038, 0400, LO, "Patient's Institution Residence")
DATA_ELEM(0038, 0500, LO, "Patient State")
DATA_ELEM(0038, 4000, LT, "Visit Comments")

DATA_ELEM(003A, 0004, CS, "Waveform Originality")
DATA_ELEM(003A, 0005, US, "Number of Waveform Channels")
DATA_ELEM(003A, 0010, UL, "Number of Waveform Samples")
DATA_ELEM(003A, 001A, DS, "Sampling Frequency")
DATA_ELEM(003A, 0020, SH, "Multiplex Group Label")
DATA_ELEM(003A, 0200, SQ, "Channel Definition Sequence")
DATA_ELEM(003A, 0202, IS, "Waveform Channel Number")
DATA_ELEM(003A, 0203, SH, "Channel Label")
DATA_ELEM(003A, 0205, CS, "Channel Status")
DATA_ELEM(003A, 0208, SQ, "Channel Source Sequence")
DATA_ELEM(003A, 0209, SQ, "Channel Source Modifiers Sequence")
DATA_ELEM(003A, 020A, SQ, "Source Waveform Sequence")
DATA_ELEM(003A, 020C, LO, "Channel Derivation Description")
DATA_ELEM(003A, 0210, DS, "Channel Sensitivity")
DATA_ELEM(003A, 0211, SQ, "Channel Sensitivity Units Sequence")
DATA_ELEM(003A, 0212, DS, "Channel Sensitivity Correction Factor")
DATA_ELEM(003A, 0213, DS, "Channel Baseline")
DATA_ELEM(003A, 0214, DS, "Channel Time Skew")
DATA_ELEM(003A, 0215, DS, "Channel Sample Skew")
DATA_ELEM(003A, 0218, DS, "Channel Offset")
DATA_ELEM(003A, 021A, US, "Waveform Bits Stored")
DATA_ELEM(003A, 0220, DS, "Filter Low Frequency")
DATA_ELEM(003A, 0221, DS, "Filter High Frequency")
DATA_ELEM(003A, 0222, DS, "Notch Filter Frequency")
DATA_ELEM(003A, 0223, DS, "Notch Filter Bandwidth")

DATA_ELEM(0040, 0001, AE, "Scheduled Station AE Title")
DATA_ELEM(0040, 0002, DA, "Scheduled Procedure Step Start Date")
DATA_ELEM(0040, 0003, TM, "Scheduled Procedure Step Start Time")
DATA_ELEM(0040, 0004, DA, "Scheduled Procedure Step End Date")
DATA_ELEM(0040, 0005, TM, "Scheduled Procedure Step End Time")
DATA_ELEM(0040, 0006, PN, "Scheduled Performing Physician's Name")
DATA_ELEM(0040, 0007, LO, "Scheduled Procedure Step Description")
DATA_ELEM(0040, 0008, SQ, "Scheduled Action Item Code Sequence")
DATA_ELEM(0040, 0009, SH, "Scheduled Procedure Step ID")
DATA_ELEM(0040, 0010, SH, "Scheduled Station Name")
DATA_ELEM(0040, 0011, SH, "Scheduled Procedure Step Location")
DATA_ELEM(0040, 0012, LO, "Pre-Medication")
DATA_ELEM(0040, 0020, CS, "Scheduled Procedure Step Status")
DATA_ELEM(0040, 0100, SQ, "Scheduled Procedure Step Sequence")
DATA_ELEM(0040, 0220, SQ, "Referenced Standalone SOP Instance Sequence")
DATA_ELEM(0040, 0241, AE, "Performed Station AE Title")
DATA_ELEM(0040, 0242, SH, "Performed Station Name")
DATA_ELEM(0040, 0243, SH, "Performed Location")
DATA_ELEM(0040, 0244, DA, "Performed Procedure Step Start Date")
DATA_ELEM(0040, 0245, TM, "Performed Procedure Step Start Time")
DATA_ELEM(0040, 0250, DA, "Performed Procedure Step End Date")
DATA_ELEM(0040, 0251, TM, "Performed Procedure Step End Time")
DATA_ELEM(0040, 0252, CS, "Performed Procedure Step Status")
DATA_ELEM(0040, 0253, SH, "Performed Procedure Step ID")
DATA_ELEM(0040, 0254, LO, "Performed Procedure Step Description")
DATA_ELEM(0040, 0255, LO, "Performed Procedure Type Description")
DATA_ELEM(0040, 0260, SQ, "Performed Action Item Sequence")
DATA_ELEM(0040, 0270, SQ, "Scheduled Step Attributes Sequence")
DATA_ELEM(0040, 0275, SQ, "Request Attributes Sequence")
DATA_ELEM(0040, 0280, ST, "Comments on the Performed Procedure Steps")
DATA_ELEM(0040, 0293, SQ, "Quantity Sequence")
DATA_ELEM(0040, 0294, DS, "Quantity")
DATA_ELEM(0040, 0295, SQ, "Measuring Units Sequence")
DATA_ELEM(0040, 0296, SQ, "Billing Item Sequence")
DATA_ELEM(0040, 0300, US, "Total Time of Fluoroscopy")
DATA_ELEM(0040, 0301, US, "Total Number of Exposures")
DATA_ELEM(0040, 0302, US, "Entrance Dose")
DATA_ELEM(0040, 0303, US, "Exposed Area")
DATA_ELEM(0040, 0306, DS, "Distance Source to Entrance")
DATA_ELEM(0040, 0307, DS, "Distance Source to Support")
DATA_ELEM(0040, 0310, ST, "Comments on Radiation Dose")
DATA_ELEM(0040, 0312, DS, "X-Ray Output")
DATA_ELEM(0040, 0314, DS, "Half Value Layer")
DATA_ELEM(0040, 0316, DS, "Organ Dose")
DATA_ELEM(0040, 0318, CS, "Organ Exposed")
DATA_ELEM(0040, 0320, SQ, "Billing Procedure Step Sequence")
DATA_ELEM(0040, 0321, SQ, "Film Consumption Sequence")
DATA_ELEM(0040, 0324, SQ, "Billing Supplies and Devices Sequence")
DATA_ELEM(0040, 0330, SQ, "Referenced Procedure Step Sequence")
DATA_ELEM(0040, 0340, SQ, "Performed Series Sequence")
DATA_ELEM(0040, 0400, LT, "Comments on the Scheduled Procedure Step")
DATA_ELEM(0040, 050A, LO, "Specimen Accession Number")
DATA_ELEM(0040, 0550, SQ, "Specimen Sequence")
DATA_ELEM(0040, 0551, LO, "Specimen Identifier")
DATA_ELEM(0040, 059A, SQ, "Specimen Type Code Sequence")
DATA_ELEM(0040, 0555, SQ, "Acquisition Context Sequence")
DATA_ELEM(0040, 0556, ST, "Acquisition Context Description")
DATA_ELEM(0040, 06FA, LO, "Slide Identifier")
DATA_ELEM(0040, 071A, SQ, "Image Center Point Coordinates Sequence")
DATA_ELEM(0040, 072A, DS, "X offset in Slide Coordinate System")
DATA_ELEM(0040, 073A, DS, "Y offset in Slide Coordinate System")
DATA_ELEM(0040, 074A, DS, "Z offset in Slide Coordinate System")
DATA_ELEM(0040, 08D8, SQ, "Pixel Spacing Sequence")
DATA_ELEM(0040, 08DA, SQ, "Coordinate System Axis Code Sequence")
DATA_ELEM(0040, 08EA, SQ, "Measurement Units Code Sequence")
DATA_ELEM(0040, 1001, SH, "Requested Procedure ID")
DATA_ELEM(0040, 1002, LO, "Reason for the Requested Procedure")
DATA_ELEM(0040, 1003, SH, "Requested Procedure Priority")
DATA_ELEM(0040, 1004, LO, "Patient Transport Arrangements")
DATA_ELEM(0040, 1005, LO, "Requested Procedure Location")
DATA_ELEM(0040, 1006, SH, "Placer Order Number / Procedure (RET)")
DATA_ELEM(0040, 1007, SH, "Filler Order Number / Procedure (RET)")
DATA_ELEM(0040, 1008, LO, "Confidentiality Code")
DATA_ELEM(0040, 1009, SH, "Reporting Priority")
DATA_ELEM(0040, 1010, PN, "Names of Intended Recipients of Results")
DATA_ELEM(0040, 1101, SQ, "Person Identification Code Sequence")
DATA_ELEM(0040, 1102, ST, "Person’s Address")
DATA_ELEM(0040, 1103, LO, "Person’s Telephone Numbers")
DATA_ELEM(0040, 1400, LT, "Requested Procedure Comments")
DATA_ELEM(0040, 2001, LO, "Reason for the Imaging Service Request")
DATA_ELEM(0040, 2004, DA, "Issue Date of Imaging Service Request")
DATA_ELEM(0040, 2005, TM, "Issue Time of Imaging Service Request")
DATA_ELEM(0040, 2006, SH, "Placer Order Number / Imaging Service Request (RET)")
DATA_ELEM(0040, 2007, SH, "Filler Order Number / Imaging Service Request (RET)")
DATA_ELEM(0040, 2008, PN, "Order Entered By")
DATA_ELEM(0040, 2009, SH, "Order Enterer's Location")
DATA_ELEM(0040, 2010, SH, "Order Callback Phone Number")
DATA_ELEM(0040, 2016, LO, "Placer Order Number / Imaging Service Request")
DATA_ELEM(0040, 2017, LO, "Filler Order Number / Imaging Service Request")
DATA_ELEM(0040, 2400, LT, "Imaging Service Request Comments")
DATA_ELEM(0040, 3001, LO, "Confidentiality Constraint on Patient Data Description")
DATA_ELEM(0040, 8302, DS, "Entrance Dose in mGy")
DATA_ELEM(0040, A010, CS, "Relationship Type")
DATA_ELEM(0040, A027, LO, "Verifying Organization")
DATA_ELEM(0040, A030, DT, "Verification DateTime")
DATA_ELEM(0040, A032, DT, "Observation DateTime")
DATA_ELEM(0040, A040, CS, "Value Type")
DATA_ELEM(0040, A043, SQ, "Concept-name Code Sequence")
DATA_ELEM(0040, A050, CS, "Continuity Of Content")
DATA_ELEM(0040, A073, SQ, "Verifying Observer Sequence")
DATA_ELEM(0040, A075, PN, "Verifying Observer Name")
DATA_ELEM(0040, A088, SQ, "Verifying Observer Identification Code Sequence")
DATA_ELEM(0040, A0B0, US, "Referenced Waveform Channels")
DATA_ELEM(0040, A120, DT, "DateTime")
DATA_ELEM(0040, A121, DA, "Date")
DATA_ELEM(0040, A122, TM, "Time")
DATA_ELEM(0040, A123, PN, "Person Name")
DATA_ELEM(0040, A124, UI, "UID")
DATA_ELEM(0040, A130, CS, "Temporal Range Type")
DATA_ELEM(0040, A132, UL, "Referenced Sample Positions")
DATA_ELEM(0040, A136, US, "Referenced Frame Numbers")
DATA_ELEM(0040, A138, DS, "Referenced Time Offsets")
DATA_ELEM(0040, A13A, DT, "Referenced Datetime")
DATA_ELEM(0040, A160, UT, "Text Value")
DATA_ELEM(0040, A168, SQ, "Concept Code Sequence")
DATA_ELEM(0040, A170, SQ, "Purpose of Reference Code Sequence")
DATA_ELEM(0040, A180, US, "Annotation Group Number")
DATA_ELEM(0040, A195, SQ, "Modifier Code Sequence")
DATA_ELEM(0040, A300, SQ, "Measured Value Sequence")
DATA_ELEM(0040, A30A, DS, "Numeric Value")
DATA_ELEM(0040, A360, SQ, "Predecessor Documents Sequence")
DATA_ELEM(0040, A370, SQ, "Referenced Request Sequence")
DATA_ELEM(0040, A372, SQ, "Performed Procedure Code Sequence")
DATA_ELEM(0040, A375, SQ, "Current Requested Procedure Evidence Sequence")
DATA_ELEM(0040, A385, SQ, "Pertinent Other Evidence Sequence")
DATA_ELEM(0040, A491, CS, "Completion Flag")
DATA_ELEM(0040, A492, LO, "Completion Flag Description")
DATA_ELEM(0040, A493, CS, "Verification Flag")
DATA_ELEM(0040, A504, SQ, "Content Template Sequence")
DATA_ELEM(0040, A525, SQ, "Identical Documents Sequence")
DATA_ELEM(0040, A730, SQ, "Content Sequence")
DATA_ELEM(0040, B020, SQ, "Annotation Sequence")
DATA_ELEM(0040, DB00, CS, "Template Identifier")
DATA_ELEM(0040, DB06, DT, "Template Version")
DATA_ELEM(0040, DB07, DT, "Template Local Version")
DATA_ELEM(0040, DB0B, CS, "Template Extension Flag")
DATA_ELEM(0040, DB0C, UI, "Template Extension Organization UID")
DATA_ELEM(0040, DB0D, UI, "Template Extension Creator UID")
DATA_ELEM(0040, DB73, UL, "Referenced Content Item Identifier")

DATA_ELEM(0050, 0004, CS, "Calibration Image")
DATA_ELEM(0050, 0010, SQ, "Device Sequence")
DATA_ELEM(0050, 0014, DS, "Device Length")
DATA_ELEM(0050, 0016, DS, "Device Diameter")
DATA_ELEM(0050, 0017, CS, "Device Diameter Units")
DATA_ELEM(0050, 0018, DS, "Device Volume")
DATA_ELEM(0050, 0019, DS, "Inter-marker Distance")
DATA_ELEM(0050, 0020, LO, "Device Description")

DATA_ELEM(0054, 0010, US, "Energy Window Vector")
DATA_ELEM(0054, 0011, US, "Number of Energy Windows")
DATA_ELEM(0054, 0012, SQ, "Energy Window Information Sequence")
DATA_ELEM(0054, 0013, SQ, "Energy Window Range Sequence")
DATA_ELEM(0054, 0014, DS, "Energy Window Lower Limit")
DATA_ELEM(0054, 0015, DS, "Energy Window Upper Limit")
DATA_ELEM(0054, 0016, SQ, "Radiopharmaceutical Information Sequence")
DATA_ELEM(0054, 0017, IS, "Residual Syringe Counts")
DATA_ELEM(0054, 0018, SH, "Energy Window Name")
DATA_ELEM(0054, 0020, US, "Detector Vector")
DATA_ELEM(0054, 0021, US, "Number of Detectors")
DATA_ELEM(0054, 0022, SQ, "Detector Information Sequence")
DATA_ELEM(0054, 0030, US, "Phase Vector")
DATA_ELEM(0054, 0031, US, "Number of Phases")
DATA_ELEM(0054, 0032, SQ, "Phase Information Sequence")
DATA_ELEM(0054, 0033, US, "Number of Frames in Phase")
DATA_ELEM(0054, 0036, IS, "Phase Delay")
DATA_ELEM(0054, 0038, IS, "Pause Between Frames")
DATA_ELEM(0054, 0050, US, "Rotation Vector")
DATA_ELEM(0054, 0051, US, "Number of Rotations")
DATA_ELEM(0054, 0052, SQ, "Rotation Information Sequence")
DATA_ELEM(0054, 0053, US, "Number of Frames in Rotation")
DATA_ELEM(0054, 0060, US, "R-R Interval Vector")
DATA_ELEM(0054, 0061, US, "Number of R-R Intervals")
DATA_ELEM(0054, 0062, SQ, "Gated Information Sequence")
DATA_ELEM(0054, 0063, SQ, "Data Information Sequence")
DATA_ELEM(0054, 0070, US, "Time Slot Vector")
DATA_ELEM(0054, 0071, US, "Number of Time Slots")
DATA_ELEM(0054, 0072, SQ, "Time Slot Information Sequence")
DATA_ELEM(0054, 0073, DS, "Time Slot Time")
DATA_ELEM(0054, 0080, US, "Slice Vector")
DATA_ELEM(0054, 0081, US, "Number of Slices")
DATA_ELEM(0054, 0090, US, "Angular View Vector")
DATA_ELEM(0054, 0100, US, "Time Slice Vector")
DATA_ELEM(0054, 0101, US, "Number of Time Slices")
DATA_ELEM(0054, 0200, DS, "Start Angle")
DATA_ELEM(0054, 0202, CS, "Type of Detector Motion")
DATA_ELEM(0054, 0210, IS, "Trigger Vector")
DATA_ELEM(0054, 0211, US, "Number of Triggers in Phase")
DATA_ELEM(0054, 0220, SQ, "View Code Sequence")
DATA_ELEM(0054, 0222, SQ, "View Modifier Code Sequence")
DATA_ELEM(0054, 0300, SQ, "Radionuclide Code Sequence")
DATA_ELEM(0054, 0302, SQ, "Administration Route Code Sequence")
DATA_ELEM(0054, 0304, SQ, "Radiopharmaceutical Code Sequence")
DATA_ELEM(0054, 0306, SQ, "Calibration Data Sequence")
DATA_ELEM(0054, 0308, US, "Energy Window Number")
DATA_ELEM(0054, 0400, SH, "Image ID")
DATA_ELEM(0054, 0410, SQ, "Patient Orientation Code Sequence")
DATA_ELEM(0054, 0412, SQ, "Patient Orientation Modifier Code Sequence")
DATA_ELEM(0054, 0414, SQ, "Patient Gantry Relationship Code Sequence")
DATA_ELEM(0054, 1000, CS, "Series Type")
DATA_ELEM(0054, 1001, CS, "Units")
DATA_ELEM(0054, 1002, CS, "Counts Source")
DATA_ELEM(0054, 1004, CS, "Reprojection Method")
DATA_ELEM(0054, 1100, CS, "Randoms Correction Method")
DATA_ELEM(0054, 1101, LO, "Attenuation Correction Method")
DATA_ELEM(0054, 1102, CS, "Decay Correction")
DATA_ELEM(0054, 1103, LO, "Reconstruction Method")
DATA_ELEM(0054, 1104, LO, "Detector Lines of Response Used")
DATA_ELEM(0054, 1105, LO, "Scatter Correction Method")
DATA_ELEM(0054, 1200, DS, "Axial Acceptance")
DATA_ELEM(0054, 1201, IS, "Axial Mash")
DATA_ELEM(0054, 1202, IS, "Transverse Mash")
DATA_ELEM(0054, 1203, DS, "Detector Element Size")
DATA_ELEM(0054, 1210, DS, "Coincidence Window Width")
DATA_ELEM(0054, 1220, CS, "Secondary Counts Type")
DATA_ELEM(0054, 1300, DS, "Frame Reference Time")
DATA_ELEM(0054, 1310, IS, "Primary (Prompts) Counts Accumulated")
DATA_ELEM(0054, 1311, IS, "Secondary Counts Accumulated")
DATA_ELEM(0054, 1320, DS, "Slice Sensitivity Factor")
DATA_ELEM(0054, 1321, DS, "Decay Factor")
DATA_ELEM(0054, 1322, DS, "Dose Calibration Factor")
DATA_ELEM(0054, 1323, DS, "Scatter Fraction Factor")
DATA_ELEM(0054, 1324, DS, "Dead Time Factor")
DATA_ELEM(0054, 1330, US, "Image Index")
DATA_ELEM(0054, 1400, CS, "Counts Included")
DATA_ELEM(0054, 1401, CS, "Dead Time Correction Flag")

DATA_ELEM(0060, 3000, SQ, "Histogram Sequence")
DATA_ELEM(0060, 3002, US, "Histogram Number of Bins")
DATA_ELEM(0060, 3004, XS, "Histogram First Bin Value")
DATA_ELEM(0060, 3006, XS, "Histogram Last Bin Value")
DATA_ELEM(0060, 3008, US, "Histogram Bin Width")
DATA_ELEM(0060, 3010, LO, "Histogram Explanation")
DATA_ELEM(0060, 3020, UL, "Histogram Data")

DATA_ELEM(0070, 0001, SQ, "Graphic Annotation Sequence")
DATA_ELEM(0070, 0002, CS, "Graphic Layer")
DATA_ELEM(0070, 0003, CS, "Bounding Box Annotation Units")
DATA_ELEM(0070, 0004, CS, "Anchor Point Annotation Units")
DATA_ELEM(0070, 0005, CS, "Graphic Annotation Units")
DATA_ELEM(0070, 0006, ST, "Unformatted Text Value")
DATA_ELEM(0070, 0008, SQ, "Text Object Sequence")
DATA_ELEM(0070, 0009, SQ, "Graphic Object Sequence")
DATA_ELEM(0070, 0010, FL, "Bounding Box Top Left Hand Corner")
DATA_ELEM(0070, 0011, FL, "Bounding Box Bottom Right Hand Corner")
DATA_ELEM(0070, 0012, CS, "Bounding Box Text Horizontal Justification")
DATA_ELEM(0070, 0014, FL, "Anchor Point")
DATA_ELEM(0070, 0015, CS, "Anchor Point Visibility")
DATA_ELEM(0070, 0020, US, "Graphic Dimensions")
DATA_ELEM(0070, 0021, US, "Number of Graphic Points")
DATA_ELEM(0070, 0022, FL, "Graphic Data")
DATA_ELEM(0070, 0023, CS, "Graphic Type")
DATA_ELEM(0070, 0024, CS, "Graphic Filled")
DATA_ELEM(0070, 0041, CS, "Image Horizontal Flip")
DATA_ELEM(0070, 0042, US, "Image Rotation")
DATA_ELEM(0070, 0052, SL, "Displayed Area Top Left Hand Corner")
DATA_ELEM(0070, 0053, SL, "Displayed Area Bottom Right Hand Corner")
DATA_ELEM(0070, 005A, SQ, "Displayed Area Selection Sequence")
DATA_ELEM(0070, 0060, SQ, "Graphic Layer Sequence")
DATA_ELEM(0070, 0062, IS, "Graphic Layer Order")
DATA_ELEM(0070, 0066, US, "Graphic Layer Recommended Display Grayscale Value")
DATA_ELEM(0070, 0067, US, "Graphic Layer Recommended Display RGB Value")
DATA_ELEM(0070, 0068, LO, "Graphic Layer Description")
DATA_ELEM(0070, 0080, CS, "Presentation Label")
DATA_ELEM(0070, 0081, LO, "Presentation Description")
DATA_ELEM(0070, 0082, DA, "Presentation Creation Date")
DATA_ELEM(0070, 0083, TM, "Presentation Creation Time")
DATA_ELEM(0070, 0084, PN, "Presentation Creator's Name")
DATA_ELEM(0070, 0100, CS, "Presentation Size Mode")
DATA_ELEM(0070, 0101, DS, "Presentation Pixel Spacing")
DATA_ELEM(0070, 0102, IS, "Presentation Pixel Aspect Ratio")
DATA_ELEM(0070, 0103, FL, "Presentation Pixel Magnification Ratio")

DATA_ELEM(0088, 0130, SH, "Storage Media File-set ID")
DATA_ELEM(0088, 0140, UI, "Storage Media File-set UID")
DATA_ELEM(0088, 0200, SQ, "Icon Image Sequence")
DATA_ELEM(0088, 0904, LO, "Topic Title")
DATA_ELEM(0088, 0906, ST, "Topic Subject")
DATA_ELEM(0088, 0910, LO, "Topic Author")
DATA_ELEM(0088, 0912, LO, "Topic Key Words")

DATA_ELEM(0100, 0410, CS, "SOP Instance Status")
DATA_ELEM(0100, 0420, DT, "SOP Authorization Date and Time")
DATA_ELEM(0100, 0424, LT, "SOP Authorization Comment")
DATA_ELEM(0100, 0426, LO, "Authorization Equipment Certification Number")

DATA_ELEM(0400, 0005, US, "MAC ID Number")
DATA_ELEM(0400, 0010, UI, "MAC Calculation Transfer Syntax UID")
DATA_ELEM(0400, 0015, CS, "MAC Algorithm")
DATA_ELEM(0400, 0020, AT, "Data Elements Signed")
DATA_ELEM(0400, 0100, UI, "Digital Signature UID")
DATA_ELEM(0400, 0105, DT, "Digital Signature DateTime")
DATA_ELEM(0400, 0110, CS, "Certificate Type")
DATA_ELEM(0400, 0115, OB, "Certificate of Signer")
DATA_ELEM(0400, 0120, OB, "Signature")
DATA_ELEM(0400, 0305, CS, "Certified Timestamp Type")
DATA_ELEM(0400, 0310, OB, "Certified Timestamp")
DATA_ELEM(0400, 0500, SQ, "Encrypted Attributes Sequence")
DATA_ELEM(0400, 0510, UI, "Encrypted Content Transfer Syntax UID")
DATA_ELEM(0400, 0520, OB, "Encrypted Content")
DATA_ELEM(0400, 0550, SQ, "Modified Attributes Sequence")

DATA_ELEM(2000, 0010, IS, "Number of Copies")
DATA_ELEM(2000, 001E, SQ, "Printer Configuration Sequence")
DATA_ELEM(2000, 0020, CS, "Print Priority")
DATA_ELEM(2000, 0030, CS, "Medium Type")
DATA_ELEM(2000, 0040, CS, "Film Destination")
DATA_ELEM(2000, 0050, LO, "Film Session Label")
DATA_ELEM(2000, 0060, IS, "Memory Allocation")
DATA_ELEM(2000, 0061, IS, "Maximum Memory Allocation")
DATA_ELEM(2000, 0062, CS, "Color Image Printing Flag")
DATA_ELEM(2000, 0063, CS, "Collation Flag")
DATA_ELEM(2000, 0065, CS, "Annotation Flag")
DATA_ELEM(2000, 0067, CS, "Image Overlay Flag")
DATA_ELEM(2000, 0069, CS, "Presentation LUT Flag")
DATA_ELEM(2000, 006A, CS, "Image Box Presentation LUT Flag")
DATA_ELEM(2000, 00A0, US, "Memory Bit Depth")
DATA_ELEM(2000, 00A1, US, "Printing Bit Depth")
DATA_ELEM(2000, 00A2, SQ, "Media Installed Sequence")
DATA_ELEM(2000, 00A4, SQ, "Other Media Available Sequence")
DATA_ELEM(2000, 00A8, SQ, "Supported Image Display Formats Sequence")
DATA_ELEM(2000, 0500, SQ, "Referenced Film Box Sequence")
DATA_ELEM(2000, 0510, SQ, "Referenced Stored Print Sequence")

DATA_ELEM(2010, 0010, ST, "Image Display Format")
DATA_ELEM(2010, 0030, CS, "Annotation Display Format ID")
DATA_ELEM(2010, 0040, CS, "Film Orientation")
DATA_ELEM(2010, 0050, CS, "Film Size ID")
DATA_ELEM(2010, 0052, CS, "Printer Resolution ID")
DATA_ELEM(2010, 0054, CS, "Default Printer Resolution ID")
DATA_ELEM(2010, 0060, CS, "Magnification Type")
DATA_ELEM(2010, 0080, CS, "Smoothing Type")
DATA_ELEM(2010, 00A6, CS, "Default Magnification Type")
DATA_ELEM(2010, 00A7, CS, "Other Magnification Types Available")
DATA_ELEM(2010, 00A8, CS, "Default Smoothing Type")
DATA_ELEM(2010, 00A9, CS, "Other Smoothing Types Available")
DATA_ELEM(2010, 0100, CS, "Border Density")
DATA_ELEM(2010, 0110, CS, "Empty Image Density")
DATA_ELEM(2010, 0120, US, "Min Density")
DATA_ELEM(2010, 0130, US, "Max Density")
DATA_ELEM(2010, 0140, CS, "Trim")
DATA_ELEM(2010, 0150, ST, "Configuration Information")
DATA_ELEM(2010, 0152, LT, "Configuration Information Description")
DATA_ELEM(2010, 0154, IS, "Maximum Collated Films")
DATA_ELEM(2010, 015E, US, "Illumination")
DATA_ELEM(2010, 0160, US, "Reflected Ambient Light")
DATA_ELEM(2010, 0376, DS, "Printer Pixel Spacing")
DATA_ELEM(2010, 0500, SQ, "Referenced Film Session Sequence")
DATA_ELEM(2010, 0510, SQ, "Referenced Image Box Sequence")
DATA_ELEM(2010, 0520, SQ, "Referenced Basic Annotation Box Sequence")

DATA_ELEM(2020, 0010, US, "Image Position")
DATA_ELEM(2020, 0020, CS, "Polarity")
DATA_ELEM(2020, 0030, DS, "Requested Image Size")
DATA_ELEM(2020, 0040, CS, "Requested Decimate/Crop Behavior")
DATA_ELEM(2020, 0050, CS, "Requested Resolution ID")
DATA_ELEM(2020, 00A0, CS, "Requested Image Size Flag")
DATA_ELEM(2020, 00A2, CS, "Decimate/Crop Result")
DATA_ELEM(2020, 0110, SQ, "Basic Grayscale Image Sequence")
DATA_ELEM(2020, 0111, SQ, "Basic Color Image Sequence")
DATA_ELEM(2020, 0130, SQ, "Referenced Image Overlay Box Sequence (RET)")
DATA_ELEM(2020, 0140, SQ, "Referenced VOI LUT Box Sequence (RET)")

DATA_ELEM(2030, 0010, US, "Annotation Position")
DATA_ELEM(2030, 0020, LO, "Text String")

DATA_ELEM(2040, 0010, SQ, "Referenced Overlay Plane Sequence")
DATA_ELEM(2040, 0011, US, "Referenced Overlay Plane Groups")
DATA_ELEM(2040, 0020, SQ, "Overlay Pixel Data Sequence")
DATA_ELEM(2040, 0060, CS, "Overlay Magnification Type")
DATA_ELEM(2040, 0070, CS, "Overlay Smoothing Type")
DATA_ELEM(2040, 0072, CS, "Overlay or Image Magnification")
DATA_ELEM(2040, 0074, US, "Magnify to Number of Columns")
DATA_ELEM(2040, 0080, CS, "Overlay Foreground Density")
DATA_ELEM(2040, 0082, CS, "Overlay Background Density")
DATA_ELEM(2040, 0090, CS, "Overlay Mode (RET)")
DATA_ELEM(2040, 0100, CS, "Threshold Density (RET)")
DATA_ELEM(2040, 0500, SQ, "Referenced Image Box Sequence (RET)")

DATA_ELEM(2050, 0010, SQ, "Presentation LUT Sequence")
DATA_ELEM(2050, 0020, CS, "Presentation LUT Shape")
DATA_ELEM(2050, 0500, SQ, "Referenced Presentation LUT Sequence")

DATA_ELEM(2100, 0010, SH, "Print Job ID")
DATA_ELEM(2100, 0020, CS, "Execution Status")
DATA_ELEM(2100, 0030, CS, "Execution Status Info")
DATA_ELEM(2100, 0040, DA, "Creation Date")
DATA_ELEM(2100, 0050, TM, "Creation Time")
DATA_ELEM(2100, 0070, AE, "Originator")
DATA_ELEM(2100, 0140, AE, "Destination AE")
DATA_ELEM(2100, 0160, SH, "Owner ID")
DATA_ELEM(2100, 0170, IS, "Number of Films")
DATA_ELEM(2100, 0500, SQ, "Referenced Print Job Sequence")

DATA_ELEM(2110, 0010, CS, "Printer Status")
DATA_ELEM(2110, 0020, CS, "Printer Status Info")
DATA_ELEM(2110, 0030, LO, "Printer Name")
DATA_ELEM(2110, 0099, SH, "Print Queue ID")

DATA_ELEM(2120, 0010, CS, "Queue Status")
DATA_ELEM(2120, 0050, SQ, "Print Job Description Sequence")
DATA_ELEM(2120, 0070, SQ, "Referenced Print Job Sequence")

DATA_ELEM(2130, 0010, SQ, "Print Management Capabilities Sequence")
DATA_ELEM(2130, 0015, SQ, "Printer Characteristics Sequence")
DATA_ELEM(2130, 0030, SQ, "Film Box Content Sequence")
DATA_ELEM(2130, 0040, SQ, "Image Box Content Sequence")
DATA_ELEM(2130, 0050, SQ, "Annotation Content Sequence")
DATA_ELEM(2130, 0060, SQ, "Image Overlay Box Content Sequence")
DATA_ELEM(2130, 0080, SQ, "Presentation LUT Content Sequence")
DATA_ELEM(2130, 00A0, SQ, "Proposed Study Sequence")
DATA_ELEM(2130, 00C0, SQ, "Original Image Sequence")

DATA_ELEM(3002, 0002, SH, "RT Image Label")
DATA_ELEM(3002, 0003, LO, "RT Image Name")
DATA_ELEM(3002, 0004, ST, "RT Image Description")
DATA_ELEM(3002, 000A, CS, "Reported Values Origin")
DATA_ELEM(3002, 000C, CS, "RT Image Plane")
DATA_ELEM(3002, 000D, DS, "X-Ray Image Receptor Translation")
DATA_ELEM(3002, 000E, DS, "X-Ray Image Receptor Angle")
DATA_ELEM(3002, 0010, DS, "RT Image Orientation")
DATA_ELEM(3002, 0011, DS, "Image Plane Pixel Spacing")
DATA_ELEM(3002, 0012, DS, "RT Image Position")
DATA_ELEM(3002, 0020, SH, "Radiation Machine Name")
DATA_ELEM(3002, 0022, DS, "Radiation Machine SAD")
DATA_ELEM(3002, 0024, DS, "Radiation Machine SSD")
DATA_ELEM(3002, 0026, DS, "RT Image SID")
DATA_ELEM(3002, 0028, DS, "Source to Reference Object Distance")
DATA_ELEM(3002, 0029, IS, "Fraction Number")
DATA_ELEM(3002, 0030, SQ, "Exposure Sequence")
DATA_ELEM(3002, 0032, DS, "Meterset Exposure")

DATA_ELEM(3004, 0001, CS, "DVH Type")
DATA_ELEM(3004, 0002, CS, "Dose Units")
DATA_ELEM(3004, 0004, CS, "Dose Type")
DATA_ELEM(3004, 0006, LO, "Dose Comment")
DATA_ELEM(3004, 0008, DS, "Normalization Point")
DATA_ELEM(3004, 000A, CS, "Dose Summation Type")
DATA_ELEM(3004, 000C, DS, "Grid Frame Offset Vector")
DATA_ELEM(3004, 000E, DS, "Dose Grid Scaling")
DATA_ELEM(3004, 0010, SQ, "RT Dose ROI Sequence")
DATA_ELEM(3004, 0012, DS, "Dose Value")
DATA_ELEM(3004, 0040, DS, "DVH Normalization Point")
DATA_ELEM(3004, 0042, DS, "DVH Normalization Dose Value")
DATA_ELEM(3004, 0050, SQ, "DVH Sequence")
DATA_ELEM(3004, 0052, DS, "DVH Dose Scaling")
DATA_ELEM(3004, 0054, CS, "DVH Volume Units")
DATA_ELEM(3004, 0056, IS, "DVH Number of Bins")
DATA_ELEM(3004, 0058, DS, "DVH Data")
DATA_ELEM(3004, 0060, SQ, "DVH Referenced ROI Sequence")
DATA_ELEM(3004, 0062, CS, "DVH ROI Contribution Type")
DATA_ELEM(3004, 0070, DS, "DVH Minimum Dose")
DATA_ELEM(3004, 0072, DS, "DVH Maximum Dose")
DATA_ELEM(3004, 0074, DS, "DVH Mean Dose")

DATA_ELEM(3006, 0002, SH, "Structure Set Label")
DATA_ELEM(3006, 0004, LO, "Structure Set Name")
DATA_ELEM(3006, 0006, ST, "Structure Set Description")
DATA_ELEM(3006, 0008, DA, "Structure Set Date")
DATA_ELEM(3006, 0009, TM, "Structure Set Time")
DATA_ELEM(3006, 0010, SQ, "Referenced Frame of Reference Sequence")
DATA_ELEM(3006, 0012, SQ, "RT Referenced Study Sequence")
DATA_ELEM(3006, 0014, SQ, "RT Referenced Series Sequence")
DATA_ELEM(3006, 0016, SQ, "Contour Image Sequence")
DATA_ELEM(3006, 0020, SQ, "Structure Set ROI Sequence")
DATA_ELEM(3006, 0022, IS, "ROI Number")
DATA_ELEM(3006, 0024, UI, "Referenced Frame of Reference UID")
DATA_ELEM(3006, 0026, LO, "ROI Name")
DATA_ELEM(3006, 0028, ST, "ROI Description")
DATA_ELEM(3006, 002A, IS, "ROI Display Color")
DATA_ELEM(3006, 002C, DS, "ROI Volume")
DATA_ELEM(3006, 0030, SQ, "RT Related ROI Sequence")
DATA_ELEM(3006, 0033, CS, "RT ROI Relationship")
DATA_ELEM(3006, 0036, CS, "ROI Generation Algorithm")
DATA_ELEM(3006, 0038, LO, "ROI Generation Description")
DATA_ELEM(3006, 0039, SQ, "ROI Contour Sequence")
DATA_ELEM(3006, 0040, SQ, "Contour Sequence")
DATA_ELEM(3006, 0042, CS, "Contour Geometric Type")
DATA_ELEM(3006, 0044, DS, "Contour Slab Thickness")
DATA_ELEM(3006, 0045, DS, "Contour Offset Vector")
DATA_ELEM(3006, 0046, IS, "Number of Contour Points")
DATA_ELEM(3006, 0048, IS, "Contour Number")
DATA_ELEM(3006, 0049, IS, "Attached Contours")
DATA_ELEM(3006, 0050, DS, "Contour Data")
DATA_ELEM(3006, 0080, SQ, "RT ROI Observations Sequence")
DATA_ELEM(3006, 0082, IS, "Observation Number")
DATA_ELEM(3006, 0084, IS, "Referenced ROI Number")
DATA_ELEM(3006, 0085, SH, "ROI Observation Label")
DATA_ELEM(3006, 0086, SQ, "RT ROI Identification Code Sequence")
DATA_ELEM(3006, 0088, ST, "ROI Observation Description")
DATA_ELEM(3006, 00A0, SQ, "Related RT ROI Observations Sequence")
DATA_ELEM(3006, 00A4, CS, "RT ROI Interpreted Type")
DATA_ELEM(3006, 00A6, PN, "ROI Interpreter")
DATA_ELEM(3006, 00B0, SQ, "ROI Physical Properties Sequence")
DATA_ELEM(3006, 00B2, CS, "ROI Physical Property")
DATA_ELEM(3006, 00B4, DS, "ROI Physical Property Value")
DATA_ELEM(3006, 00C0, SQ, "Frame of Reference Relationship Sequence")
DATA_ELEM(3006, 00C2, UI, "Related Frame of Reference UID")
DATA_ELEM(3006, 00C4, CS, "Frame of Reference Transformation Type")
DATA_ELEM(3006, 00C6, DS, "Frame of Reference Transformation Matrix")
DATA_ELEM(3006, 00C8, LO, "Frame of Reference Transformation Comment")

DATA_ELEM(3008, 0010, SQ, "Measured Dose Reference Sequence")
DATA_ELEM(3008, 0012, ST, "Measured Dose Description")
DATA_ELEM(3008, 0014, CS, "Measured Dose Type")
DATA_ELEM(3008, 0016, DS, "Measured Dose Value")
DATA_ELEM(3008, 0020, SQ, "Treatment Session Beam Sequence")
DATA_ELEM(3008, 0022, IS, "Current Fraction Number")
DATA_ELEM(3008, 0024, DA, "Treatment Control Point Date")
DATA_ELEM(3008, 0025, TM, "Treatment Control Point Time")
DATA_ELEM(3008, 002A, CS, "Treatment Termination Status")
DATA_ELEM(3008, 002B, SH, "Treatment Termination Code")
DATA_ELEM(3008, 002C, CS, "Treatment Verification Status")
DATA_ELEM(3008, 0030, SQ, "Referenced Treatment Record Sequence")
DATA_ELEM(3008, 0032, DS, "Specified Primary Meterset")
DATA_ELEM(3008, 0033, DS, "Specified Secondary Meterset")
DATA_ELEM(3008, 0036, DS, "Delivered Primary Meterset")
DATA_ELEM(3008, 0037, DS, "Delivered Secondary Meterset")
DATA_ELEM(3008, 003A, DS, "Specified Treatment Time")
DATA_ELEM(3008, 003B, DS, "Delivered Treatment Time")
DATA_ELEM(3008, 0040, SQ, "Control Point Delivery Sequence")
DATA_ELEM(3008, 0042, DS, "Specified Meterset")
DATA_ELEM(3008, 0044, DS, "Delivered Meterset")
DATA_ELEM(3008, 0048, DS, "Dose Rate Delivered")
DATA_ELEM(3008, 0050, SQ, "Treatment Summary Calculated Dose Reference Sequence")
DATA_ELEM(3008, 0052, DS, "Cumulative Dose to Dose Reference")
DATA_ELEM(3008, 0054, DA, "First Treatment Date")
DATA_ELEM(3008, 0056, DA, "Most Recent Treatment Date")
DATA_ELEM(3008, 005A, IS, "Number of Fractions Delivered")
DATA_ELEM(3008, 0060, SQ, "Override Sequence")
DATA_ELEM(3008, 0062, AT, "Override Parameter Pointer")
DATA_ELEM(3008, 0064, IS, "Measured Dose Reference Number")
DATA_ELEM(3008, 0066, ST, "Override Reason")
DATA_ELEM(3008, 0070, SQ, "Calculated Dose Reference Sequence")
DATA_ELEM(3008, 0072, IS, "Calculated Dose Reference Number")
DATA_ELEM(3008, 0074, ST, "Calculated Dose Reference Description")
DATA_ELEM(3008, 0076, DS, "Calculated Dose Reference Dose Value")
DATA_ELEM(3008, 0078, DS, "Start Meterset")
DATA_ELEM(3008, 007A, DS, "End Meterset")
DATA_ELEM(3008, 0080, SQ, "Referenced Measured Dose Reference Sequence")
DATA_ELEM(3008, 0082, IS, "Referenced Measured Dose Reference Number")
DATA_ELEM(3008, 0090, SQ, "Referenced Calculated Dose Reference Sequence")
DATA_ELEM(3008, 0092, IS, "Referenced Calculated Dose Reference Number")
DATA_ELEM(3008, 00A0, SQ, "Beam Limiting Device Leaf Pairs Sequence")
DATA_ELEM(3008, 00B0, SQ, "Recorded Wedge Sequence")
DATA_ELEM(3008, 00C0, SQ, "Recorded Compensator Sequence")
DATA_ELEM(3008, 00D0, SQ, "Recorded Block Sequence")
DATA_ELEM(3008, 00E0, SQ, "Treatment Summary Measured Dose Reference Sequence")
DATA_ELEM(3008, 0100, SQ, "Recorded Source Sequence")
DATA_ELEM(3008, 0105, LO, "Source Serial Number")
DATA_ELEM(3008, 0110, SQ, "Treatment Session Application Setup Sequence")
DATA_ELEM(3008, 0116, CS, "Application Setup Check")
DATA_ELEM(3008, 0120, SQ, "Recorded Brachy Accessory Device Sequence")
DATA_ELEM(3008, 0122, IS, "Referenced Brachy Accessory Device Number")
DATA_ELEM(3008, 0130, SQ, "Recorded Channel Sequence")
DATA_ELEM(3008, 0132, DS, "Specified Channel Total Time")
DATA_ELEM(3008, 0134, DS, "Delivered Channel Total Time")
DATA_ELEM(3008, 0136, IS, "Specified Number of Pulses")
DATA_ELEM(3008, 0138, IS, "Delivered Number of Pulses")
DATA_ELEM(3008, 013A, DS, "Specified Pulse Repetition Interval")
DATA_ELEM(3008, 013C, DS, "Delivered Pulse Repetition Interval")
DATA_ELEM(3008, 0140, SQ, "Recorded Source Applicator Sequence")
DATA_ELEM(3008, 0142, IS, "Referenced Source Applicator Number")
DATA_ELEM(3008, 0150, SQ, "Recorded Channel Shield Sequence")
DATA_ELEM(3008, 0152, IS, "Referenced Channel Shield Number")
DATA_ELEM(3008, 0160, SQ, "Brachy Control Point Delivered Sequence")
DATA_ELEM(3008, 0162, DA, "Safe Position Exit Date")
DATA_ELEM(3008, 0164, TM, "Safe Position Exit Time")
DATA_ELEM(3008, 0166, DA, "Safe Position Return Date")
DATA_ELEM(3008, 0168, TM, "Safe Position Return Time")
DATA_ELEM(3008, 0200, CS, "Current Treatment Status")
DATA_ELEM(3008, 0202, ST, "Treatment Status Comment")
DATA_ELEM(3008, 0220, SQ, "Fraction Group Summary Sequence")
DATA_ELEM(3008, 0223, IS, "Referenced Fraction Number")
DATA_ELEM(3008, 0224, CS, "Fraction Group Type")
DATA_ELEM(3008, 0230, CS, "Beam Stopper Position")
DATA_ELEM(3008, 0240, SQ, "Fraction Status Summary Sequence")
DATA_ELEM(3008, 0250, DA, "Treatment Date")
DATA_ELEM(3008, 0251, TM, "Treatment Time")

DATA_ELEM(300A, 0002, SH, "RT Plan Label")
DATA_ELEM(300A, 0003, LO, "RT Plan Name")
DATA_ELEM(300A, 0004, ST, "RT Plan Description")
DATA_ELEM(300A, 0006, DA, "RT Plan Date")
DATA_ELEM(300A, 0007, TM, "RT Plan Time")
DATA_ELEM(300A, 0009, LO, "Treatment Protocols")
DATA_ELEM(300A, 000A, CS, "Treatment Intent")
DATA_ELEM(300A, 000B, LO, "Treatment Sites")
DATA_ELEM(300A, 000C, CS, "RT Plan Geometry")
DATA_ELEM(300A, 000E, ST, "Prescription Description")
DATA_ELEM(300A, 0010, SQ, "Dose Reference Sequence")
DATA_ELEM(300A, 0012, IS, "Dose Reference Number")
DATA_ELEM(300A, 0014, CS, "Dose Reference Structure Type")
DATA_ELEM(300A, 0015, CS, "Nominal Beam Energy Unit")
DATA_ELEM(300A, 0016, LO, "Dose Reference Description")
DATA_ELEM(300A, 0018, DS, "Dose Reference Point Coordinates")
DATA_ELEM(300A, 001A, DS, "Nominal Prior Dose")
DATA_ELEM(300A, 0020, CS, "Dose Reference Type")
DATA_ELEM(300A, 0021, DS, "Constraint Weight")
DATA_ELEM(300A, 0022, DS, "Delivery Warning Dose")
DATA_ELEM(300A, 0023, DS, "Delivery Maximum Dose")
DATA_ELEM(300A, 0025, DS, "Target Minimum Dose")
DATA_ELEM(300A, 0026, DS, "Target Prescription Dose")
DATA_ELEM(300A, 0027, DS, "Target Maximum Dose")
DATA_ELEM(300A, 0028, DS, "Target Underdose Volume Fraction")
DATA_ELEM(300A, 002A, DS, "Organ at Risk Full-volume Dose")
DATA_ELEM(300A, 002B, DS, "Organ at Risk Limit Dose")
DATA_ELEM(300A, 002C, DS, "Organ at Risk Maximum Dose")
DATA_ELEM(300A, 002D, DS, "Organ at Risk Overdose Volume Fraction")
DATA_ELEM(300A, 0040, SQ, "Tolerance Table Sequence")
DATA_ELEM(300A, 0042, IS, "Tolerance Table Number")
DATA_ELEM(300A, 0043, SH, "Tolerance Table Label")
DATA_ELEM(300A, 0044, DS, "Gantry Angle Tolerance")
DATA_ELEM(300A, 0046, DS, "Beam Limiting Device Angle Tolerance")
DATA_ELEM(300A, 0048, SQ, "Beam Limiting Device Tolerance Sequence")
DATA_ELEM(300A, 004A, DS, "Beam Limiting Device Position Tolerance")
DATA_ELEM(300A, 004C, DS, "Patient Support Angle Tolerance")
DATA_ELEM(300A, 004E, DS, "Table Top Eccentric Angle Tolerance")
DATA_ELEM(300A, 0051, DS, "Table Top Vertical Position Tolerance")
DATA_ELEM(300A, 0052, DS, "Table Top Longitudinal Position Tolerance")
DATA_ELEM(300A, 0053, DS, "Table Top Lateral Position Tolerance")
DATA_ELEM(300A, 0055, CS, "RT Plan Relationship")
DATA_ELEM(300A, 0070, SQ, "Fraction Group Sequence")
DATA_ELEM(300A, 0071, IS, "Fraction Group Number")
DATA_ELEM(300A, 0078, IS, "Number of Fractions Planned")
DATA_ELEM(300A, 0079, IS, "Number of Fractions Per Day")
DATA_ELEM(300A, 007A, IS, "Repeat Fraction Cycle Length")
DATA_ELEM(300A, 007B, LT, "Fraction Pattern")
DATA_ELEM(300A, 0080, IS, "Number of Beams")
DATA_ELEM(300A, 0082, DS, "Beam Dose Specification Point")
DATA_ELEM(300A, 0084, DS, "Beam Dose")
DATA_ELEM(300A, 0086, DS, "Beam Meterset")
DATA_ELEM(300A, 00A0, IS, "Number of Brachy Application Setups")
DATA_ELEM(300A, 00A2, DS, "Brachy Application Setup Dose Specification Point")
DATA_ELEM(300A, 00A4, DS, "Brachy Application Setup Dose")
DATA_ELEM(300A, 00B0, SQ, "Beam Sequence")
DATA_ELEM(300A, 00B2, SH, "Treatment Machine Name")
DATA_ELEM(300A, 00B3, CS, "Primary Dosimeter Unit")
DATA_ELEM(300A, 00B4, DS, "Source-Axis Distance")
DATA_ELEM(300A, 00B6, SQ, "Beam Limiting Device Sequence")
DATA_ELEM(300A, 00B8, CS, "RT Beam Limiting Device Type")
DATA_ELEM(300A, 00BA, DS, "Source to Beam Limiting Device Distance")
DATA_ELEM(300A, 00BC, IS, "Number of Leaf/Jaw Pairs")
DATA_ELEM(300A, 00BE, DS, "Leaf Position Boundaries")
DATA_ELEM(300A, 00C0, IS, "Beam Number")
DATA_ELEM(300A, 00C2, LO, "Beam Name")
DATA_ELEM(300A, 00C3, ST, "Beam Description")
DATA_ELEM(300A, 00C4, CS, "Beam Type")
DATA_ELEM(300A, 00C6, CS, "Radiation Type")
DATA_ELEM(300A, 00C8, IS, "Reference Image Number")
DATA_ELEM(300A, 00CA, SQ, "Planned Verification Image Sequence")
DATA_ELEM(300A, 00CC, LO, "Imaging Device-Specific Acquisition Parameters")
DATA_ELEM(300A, 00CE, CS, "Treatment Delivery Type")
DATA_ELEM(300A, 00D0, IS, "Number of Wedges")
DATA_ELEM(300A, 00D1, SQ, "Wedge Sequence")
DATA_ELEM(300A, 00D2, IS, "Wedge Number")
DATA_ELEM(300A, 00D3, CS, "Wedge Type")
DATA_ELEM(300A, 00D4, SH, "Wedge ID")
DATA_ELEM(300A, 00D5, IS, "Wedge Angle")
DATA_ELEM(300A, 00D6, DS, "Wedge Factor")
DATA_ELEM(300A, 00D8, DS, "Wedge Orientation")
DATA_ELEM(300A, 00DA, DS, "Source to Wedge Tray Distance")
DATA_ELEM(300A, 00E0, IS, "Number of Compensators")
DATA_ELEM(300A, 00E1, SH, "Material ID")
DATA_ELEM(300A, 00E2, DS, "Total Compensator Tray Factor")
DATA_ELEM(300A, 00E3, SQ, "Compensator Sequence")
DATA_ELEM(300A, 00E4, IS, "Compensator Number")
DATA_ELEM(300A, 00E5, SH, "Compensator ID")
DATA_ELEM(300A, 00E6, DS, "Source to Compensator Tray Distance")
DATA_ELEM(300A, 00E7, IS, "Compensator Rows")
DATA_ELEM(300A, 00E8, IS, "Compensator Columns")
DATA_ELEM(300A, 00E9, DS, "Compensator Pixel Spacing")
DATA_ELEM(300A, 00EA, DS, "Compensator Position")
DATA_ELEM(300A, 00EB, DS, "Compensator Transmission Data")
DATA_ELEM(300A, 00EC, DS, "Compensator Thickness Data")
DATA_ELEM(300A, 00ED, IS, "Number of Boli")
DATA_ELEM(300A, 00EE, CS, "Compensator Type")
DATA_ELEM(300A, 00F0, IS, "Number of Blocks")
DATA_ELEM(300A, 00F2, DS, "Total Block Tray Factor")
DATA_ELEM(300A, 00F4, SQ, "Block Sequence")
DATA_ELEM(300A, 00F5, SH, "Block Tray ID")
DATA_ELEM(300A, 00F6, DS, "Source to Block Tray Distance")
DATA_ELEM(300A, 00F8, CS, "Block Type")
DATA_ELEM(300A, 00FA, CS, "Block Divergence")
DATA_ELEM(300A, 00FC, IS, "Block Number")
DATA_ELEM(300A, 00FE, LO, "Block Name")
DATA_ELEM(300A, 0100, DS, "Block Thickness")
DATA_ELEM(300A, 0102, DS, "Block Transmission")
DATA_ELEM(300A, 0104, IS, "Block Number of Points")
DATA_ELEM(300A, 0106, DS, "Block Data")
DATA_ELEM(300A, 0107, SQ, "Applicator Sequence")
DATA_ELEM(300A, 0108, SH, "Applicator ID")
DATA_ELEM(300A, 0109, CS, "Applicator Type")
DATA_ELEM(300A, 010A, LO, "Applicator Description")
DATA_ELEM(300A, 010C, DS, "Cumulative Dose Reference Coefficient")
DATA_ELEM(300A, 010E, DS, "Final Cumulative Meterset Weight")
DATA_ELEM(300A, 0110, IS, "Number of Control Points")
DATA_ELEM(300A, 0111, SQ, "Control Point Sequence")
DATA_ELEM(300A, 0112, IS, "Control Point Index")
DATA_ELEM(300A, 0114, DS, "Nominal Beam Energy")
DATA_ELEM(300A, 0115, DS, "Dose Rate Set")
DATA_ELEM(300A, 0116, SQ, "Wedge Position Sequence")
DATA_ELEM(300A, 0118, CS, "Wedge Position")
DATA_ELEM(300A, 011A, SQ, "Beam Limiting Device Position Sequence")
DATA_ELEM(300A, 011C, DS, "Leaf/Jaw Positions")
DATA_ELEM(300A, 011E, DS, "Gantry Angle")
DATA_ELEM(300A, 011F, CS, "Gantry Rotation Direction")
DATA_ELEM(300A, 0120, DS, "Beam Limiting Device Angle")
DATA_ELEM(300A, 0121, CS, "Beam Limiting Device Rotation Direction")
DATA_ELEM(300A, 0122, DS, "Patient Support Angle")
DATA_ELEM(300A, 0123, CS, "Patient Support Rotation Direction")
DATA_ELEM(300A, 0124, DS, "Table Top Eccentric Axis Distance")
DATA_ELEM(300A, 0125, DS, "Table Top Eccentric Angle")
DATA_ELEM(300A, 0126, CS, "Table Top Eccentric Rotation Direction")
DATA_ELEM(300A, 0128, DS, "Table Top Vertical Position")
DATA_ELEM(300A, 0129, DS, "Table Top Longitudinal Position")
DATA_ELEM(300A, 012A, DS, "Table Top Lateral Position")
DATA_ELEM(300A, 012C, DS, "Isocenter Position")
DATA_ELEM(300A, 012E, DS, "Surface Entry Point")
DATA_ELEM(300A, 0130, DS, "Source to Surface Distance")
DATA_ELEM(300A, 0134, DS, "Cumulative Meterset Weight")
DATA_ELEM(300A, 0180, SQ, "Patient Setup Sequence")
DATA_ELEM(300A, 0182, IS, "Patient Setup Number")
DATA_ELEM(300A, 0184, LO, "Patient Additional Position")
DATA_ELEM(300A, 0190, SQ, "Fixation Device Sequence")
DATA_ELEM(300A, 0192, CS, "Fixation Device Type")
DATA_ELEM(300A, 0194, SH, "Fixation Device Label")
DATA_ELEM(300A, 0196, ST, "Fixation Devi ce Description")
DATA_ELEM(300A, 0198, SH, "Fixation Device Position")
DATA_ELEM(300A, 01A0, SQ, "Shielding Device Sequence")
DATA_ELEM(300A, 01A2, CS, "Shielding Device Type")
DATA_ELEM(300A, 01A4, SH, "Shielding Device Label")
DATA_ELEM(300A, 01A6, ST, "Shielding Device Description")
DATA_ELEM(300A, 01A8, SH, "Shielding Device Position")
DATA_ELEM(300A, 01B0, CS, "Setup Technique")
DATA_ELEM(300A, 01B2, ST, "Setup Technique Description")
DATA_ELEM(300A, 01B4, SQ, "Setup Device Sequence")
DATA_ELEM(300A, 01B6, CS, "Setup Device Type")
DATA_ELEM(300A, 01B8, SH, "Setup Device Label")
DATA_ELEM(300A, 01BA, ST, "Setup Device Description")
DATA_ELEM(300A, 01BC, DS, "Setup Device Parameter")
DATA_ELEM(300A, 01D0, ST, "Setup Reference Description")
DATA_ELEM(300A, 01D2, DS, "Table Top Vertical Setup Displacement")
DATA_ELEM(300A, 01D4, DS, "Table Top Longitudinal Setup Displacement")
DATA_ELEM(300A, 01D6, DS, "Table Top Lateral Setup Displacement")
DATA_ELEM(300A, 0200, CS, "Brachy Treatment Technique")
DATA_ELEM(300A, 0202, CS, "Brachy Treatment Type")
DATA_ELEM(300A, 0206, SQ, "Treatment Machine Sequence")
DATA_ELEM(300A, 0210, SQ, "Source Sequence")
DATA_ELEM(300A, 0212, IS, "Source Number")
DATA_ELEM(300A, 0214, CS, "Source Type")
DATA_ELEM(300A, 0216, LO, "Source Manufacturer")
DATA_ELEM(300A, 0218, DS, "Active Source Diameter")
DATA_ELEM(300A, 021A, DS, "Active Source Length")
DATA_ELEM(300A, 0222, DS, "Source Encapsulation Nominal Thickness")
DATA_ELEM(300A, 0224, DS, "Source Encapsulation Nominal Transmission")
DATA_ELEM(300A, 0226, LO, "Source Isotope Name")
DATA_ELEM(300A, 0228, DS, "Source Isotope Half Life")
DATA_ELEM(300A, 022A, DS, "Reference Air Kerma Rate")
DATA_ELEM(300A, 022C, DA, "Air Kerma Rate Reference Date")
DATA_ELEM(300A, 022E, TM, "Air Kerma Rate Reference Time")
DATA_ELEM(300A, 0230, SQ, "Application Setup Sequence")
DATA_ELEM(300A, 0232, CS, "Application Setup Type")
DATA_ELEM(300A, 0234, IS, "Application Setup Number")
DATA_ELEM(300A, 0236, LO, "Application Setup Name")
DATA_ELEM(300A, 0238, LO, "Application Setup Manufacturer")
DATA_ELEM(300A, 0240, IS, "Template Number")
DATA_ELEM(300A, 0242, SH, "Template Type")
DATA_ELEM(300A, 0244, LO, "Template Name")
DATA_ELEM(300A, 0250, DS, "Total Reference Air Kerma")
DATA_ELEM(300A, 0260, SQ, "Brachy Accessory Device Sequence")
DATA_ELEM(300A, 0262, IS, "Brachy Accessory Device Number")
DATA_ELEM(300A, 0263, SH, "Brachy Accessory Device ID")
DATA_ELEM(300A, 0264, CS, "Brachy Accessory Device Type")
DATA_ELEM(300A, 0266, LO, "Brachy Accessory Device Name")
DATA_ELEM(300A, 026A, DS, "Brachy Accessory Device Nominal Thickness")
DATA_ELEM(300A, 026C, DS, "Brachy Accessory Device Nominal Transmission")
DATA_ELEM(300A, 0280, SQ, "Channel Sequence")
DATA_ELEM(300A, 0282, IS, "Channel Number")
DATA_ELEM(300A, 0284, DS, "Channel Length")
DATA_ELEM(300A, 0286, DS, "Channel Total Time")
DATA_ELEM(300A, 0288, CS, "Source Movement Type")
DATA_ELEM(300A, 028A, IS, "Number of Pulses")
DATA_ELEM(300A, 028C, DS, "Pulse Repetition Interval")
DATA_ELEM(300A, 0290, IS, "Source Applicator Number")
DATA_ELEM(300A, 0291, SH, "Source Applicator ID")
DATA_ELEM(300A, 0292, CS, "Source Applicator Type")
DATA_ELEM(300A, 0294, LO, "Source Applicator Name")
DATA_ELEM(300A, 0296, DS, "Source Applicator Length")
DATA_ELEM(300A, 0298, LO, "Source Applicator Manufacturer")
DATA_ELEM(300A, 029C, DS, "Source Applicator Wall Nominal Thickness")
DATA_ELEM(300A, 029E, DS, "Source Applicator Wall Nominal Transmission")
DATA_ELEM(300A, 02A0, DS, "Source Applicator Step Size")
DATA_ELEM(300A, 02A2, IS, "Transfer Tube Number")
DATA_ELEM(300A, 02A4, DS, "Transfer Tube Length")
DATA_ELEM(300A, 02B0, SQ, "Channel Shield Sequence")
DATA_ELEM(300A, 02B2, IS, "Channel Shield Number")
DATA_ELEM(300A, 02B3, SH, "Channel Shield ID")
DATA_ELEM(300A, 02B4, LO, "Channel Shield Name")
DATA_ELEM(300A, 02B8, DS, "Channel Shield Nominal Thickness")
DATA_ELEM(300A, 02BA, DS, "Channel Shield Nominal Transmission")
DATA_ELEM(300A, 02C8, DS, "Final Cumulative Time Weight")
DATA_ELEM(300A, 02D0, SQ, "Brachy Control Point Sequence")
DATA_ELEM(300A, 02D2, DS, "Control Point Relative Position")
DATA_ELEM(300A, 02D4, DS, "Control Point 3D Position")
DATA_ELEM(300A, 02D6, DS, "Cumulative Time Weight")

DATA_ELEM(300C, 0002, SQ, "Referenced RT Plan Sequence")
DATA_ELEM(300C, 0004, SQ, "Referenced Beam Sequence")
DATA_ELEM(300C, 0006, IS, "Referenced Beam Number")
DATA_ELEM(300C, 0007, IS, "Referenced Reference Image Number")
DATA_ELEM(300C, 0008, DS, "Start Cumulative Meterset Weight")
DATA_ELEM(300C, 0009, DS, "End Cumulative Meterset Weight")
DATA_ELEM(300C, 000A, SQ, "Referenced Brachy Application Setup Sequence")
DATA_ELEM(300C, 000C, IS, "Referenced Brachy Application Setup Number")
DATA_ELEM(300C, 000E, IS, "Referenced Source Number")
DATA_ELEM(300C, 0020, SQ, "Referenced Fraction Group Sequence")
DATA_ELEM(300C, 0022, IS, "Referenced Fraction Group Number")
DATA_ELEM(300C, 0040, SQ, "Referenced Verification Image Sequence")
DATA_ELEM(300C, 0042, SQ, "Referenced Reference Image Sequence")
DATA_ELEM(300C, 0050, SQ, "Referenced Dose Reference Sequence")
DATA_ELEM(300C, 0051, IS, "Referenced Dose Reference Number")
DATA_ELEM(300C, 0055, SQ, "Brachy Referenced Dose Reference Sequence")
DATA_ELEM(300C, 0060, SQ, "Referenced Structure Set Sequence")
DATA_ELEM(300C, 006A, IS, "Referenced Patient Setup Number")
DATA_ELEM(300C, 0080, SQ, "Referenced Dose Sequence")
DATA_ELEM(300C, 00A0, IS, "Referenced Tolerance Table Number")
DATA_ELEM(300C, 00B0, SQ, "Referenced Bolus Sequence")
DATA_ELEM(300C, 00C0, IS, "Referenced Wedge Number")
DATA_ELEM(300C, 00D0, IS, "Referenced Compensator Number")
DATA_ELEM(300C, 00E0, IS, "Referenced Block Number")
DATA_ELEM(300C, 00F0, IS, "Referenced Control Point Index")

DATA_ELEM(300E, 0002, CS, "Approval Status")
DATA_ELEM(300E, 0004, DA, "Review Date")
DATA_ELEM(300E, 0005, TM, "Review Time")
DATA_ELEM(300E, 0008, PN, "Reviewer Name")

DATA_ELEM(4008, 0040, SH, "Results ID")
DATA_ELEM(4008, 0042, LO, "Results ID Issuer")
DATA_ELEM(4008, 0050, SQ, "Referenced Interpretation Sequence")
DATA_ELEM(4008, 0100, DA, "Interpretation Recorded Date")
DATA_ELEM(4008, 0101, TM, "Interpretation Recorded Time")
DATA_ELEM(4008, 0102, PN, "Interpretation Recorder")
DATA_ELEM(4008, 0103, LO, "Reference to Recorded Sound")
DATA_ELEM(4008, 0108, DA, "Interpretation Transcription Date")
DATA_ELEM(4008, 0109, TM, "Interpretation Transcription Time")
DATA_ELEM(4008, 010A, PN, "Interpretation Transcriber")
DATA_ELEM(4008, 010B, ST, "Interpretation Text")
DATA_ELEM(4008, 010C, PN, "Interpretation Author")
DATA_ELEM(4008, 0111, SQ, "Interpretation Approver Sequence")
DATA_ELEM(4008, 0112, DA, "Interpretation Approval Date")
DATA_ELEM(4008, 0113, TM, "Interpretation Approval Time")
DATA_ELEM(4008, 0114, PN, "Physician Approving Interpretation")
DATA_ELEM(4008, 0115, LT, "Interpretation Diagnosis Description")
DATA_ELEM(4008, 0117, SQ, "Interpretation Diagnosis Code Sequence")
DATA_ELEM(4008, 0118, SQ, "Results Distribution List Sequence")
DATA_ELEM(4008, 0119, PN, "Distribution Name")
DATA_ELEM(4008, 011A, LO, "Distribution Address")
DATA_ELEM(4008, 0200, SH, "Interpretation ID")
DATA_ELEM(4008, 0202, LO, "Interpretation ID Issuer")
DATA_ELEM(4008, 0210, CS, "Interpretation Type ID")
DATA_ELEM(4008, 0212, CS, "Interpretation Status ID")
DATA_ELEM(4008, 0300, ST, "Impressions")
DATA_ELEM(4008, 4000, ST, "Results Comments")

DATA_ELEM(4FFE, 0001, SQ, "MAC Parameters Sequence")

DATA_ELEM(5000, 0005, US, "Curve Dimensions")
DATA_ELEM(5000, 0010, US, "Number of Points")
DATA_ELEM(5000, 0020, CS, "Type of Data")
DATA_ELEM(5000, 0022, LO, "Curve Description")
DATA_ELEM(5000, 0030, SH, "Axis Units")
DATA_ELEM(5000, 0040, SH, "Axis Labels")
DATA_ELEM(5000, 0103, US, "Data Value Representation")
DATA_ELEM(5000, 0104, US, "Minimum Coordinate Value")
DATA_ELEM(5000, 0105, US, "Maximum Coordinate Value")
DATA_ELEM(5000, 0106, SH, "Curve Range")
DATA_ELEM(5000, 0110, US, "Curve Data Descriptor")
DATA_ELEM(5000, 0112, US, "Coordinate Start Value")
DATA_ELEM(5000, 0114, US, "Coordinate Step Value")
DATA_ELEM(5000, 1001, CS, "Curve Activation Layer")
DATA_ELEM(5000, 2000, US, "Audio Type")
DATA_ELEM(5000, 2002, US, "Audio Sample Format")
DATA_ELEM(5000, 2004, US, "Number of Channels")
DATA_ELEM(5000, 2006, UL, "Number of Samples")
DATA_ELEM(5000, 2008, UL, "Sample Rate")
DATA_ELEM(5000, 200A, UL, "Total Time")
DATA_ELEM(5000, 200C, OW, "Audio Sample Data")
DATA_ELEM(5000, 200E, LT, "Audio Comments")
DATA_ELEM(5000, 2500, LO, "Curve Label")
DATA_ELEM(5000, 2600, SQ, "Referenced Overlay Sequence")
DATA_ELEM(5000, 2610, US, "Referenced Overlay Group")
DATA_ELEM(5000, 3000, OW, "Curve Data")

DATA_ELEM(5400, 0100, SQ, "Waveform Sequence")
DATA_ELEM(5400, 0110, OW, "Channel Minimum Value")
DATA_ELEM(5400, 0112, OW, "Channel Maximum Value")
DATA_ELEM(5400, 1004, US, "Waveform Bits Allocated")
DATA_ELEM(5400, 1006, CS, "Waveform Sample Interpretation")
DATA_ELEM(5400, 100A, OW, "Waveform Padding Value")
DATA_ELEM(5400, 1010, OW, "Waveform Data")

DATA_ELEM(6000, 0010, US, "Overlay Rows")
DATA_ELEM(6000, 0011, US, "Overlay Columns")
DATA_ELEM(6000, 0012, US, "Overlay Planes")
DATA_ELEM(6000, 0015, IS, "Number of Frames in Overlay")
DATA_ELEM(6000, 0022, LO, "Overlay Description")
DATA_ELEM(6000, 0040, CS, "Overlay Type")
DATA_ELEM(6000, 0045, LO, "Overlay Subtype")
DATA_ELEM(6000, 0050, SS, "Overlay Origin")
DATA_ELEM(6000, 0051, US, "Image Frame Origin")
DATA_ELEM(6000, 0052, US, "Overlay Plane Origin")
DATA_ELEM(6000, 0060, CS, "Compression Code (RET)")
DATA_ELEM(6000, 0100, US, "Overlay Bits Allocated")
DATA_ELEM(6000, 0102, US, "Overlay Bit Position")
DATA_ELEM(6000, 1001, CS, "Overlay Activation Layer")
DATA_ELEM(6000, 1100, US, "Overlay Descriptor - Gray (RET)")
DATA_ELEM(6000, 1101, US, "Overlay Descriptor - Red (RET)")
DATA_ELEM(6000, 1102, US, "Overlay Descriptor - Green (RET)")
DATA_ELEM(6000, 1103, US, "Overlay Descriptor - Blue (RET)")
DATA_ELEM(6000, 1200, US, "Overlays - Gray (RET)")
DATA_ELEM(6000, 1201, US, "Overlays - Red (RET)")
DATA_ELEM(6000, 1202, US, "Overlays - Green (RET)")
DATA_ELEM(6000, 1203, US, "Overlays - Blue (RET)")
DATA_ELEM(6000, 1301, IS, "ROI Area")
DATA_ELEM(6000, 1302, DS, "ROI Mean")
DATA_ELEM(6000, 1303, DS, "ROI Standard Deviation")
DATA_ELEM(6000, 1500, LO, "Overlay Label")
DATA_ELEM(6000, 3000, OW, "Overlay Data")
DATA_ELEM(6000, 4000, LO, "Comments (RET)")

DATA_ELEM(7FE0, 0010, OW, "Pixel Data")

DATA_ELEM(FFFA, FFFA, SQ, "Digital Signatures Sequence")

DATA_ELEM(FFFC, FFFC, OB, "Data Set Trailing Padding")

DATA_ELEM(FFFE, E000, UL, "Item")
DATA_ELEM(FFFE, E00D, UL, "Item Delimitation Item")
DATA_ELEM(FFFE, E0DD, UL, "Sequence Delimitation Item")

//========================= private elements ================

//-------------------- Marconi ------------------------------
DATA_ELEM(0029, 0060, LO, "RadWorksMarconi")
PRIVATE_ELEM(0029, 6024, US, DCM_MARCONIKEYFRAMEINDICES, "<internal>")


//-------------------- Workstation Internal ---------------------
DATA_ELEM(3101, 0010, LO, "AMI Annotations_02")
PRIVATE_ELEM(3101, 1020, SQ, DCM_AMIANNOTATIONSEQUENCE2, "AMI Annotation Sequence (RET)")

DATA_ELEM(3101, 0011, LO, "AMI Annotations_01")
PRIVATE_ELEM(3101, 1110, SQ, DCM_AMIANNOTATIONSEQUENCE, "AMI Annotation Sequence (RET)")

DATA_ELEM(3103, 0011, LO, "AMI Sequence Annotations_01")
PRIVATE_ELEM(3103, 1110, CS, DCM_AMIANNOTSEQUENCETYPE_OLD, "AMI Annotation Sequence (RET)")
PRIVATE_ELEM(3103, 1120, UI, DCM_AMIANNOTSEQUENCEUID_OLD, "AMI Annotation UID (RET)")
PRIVATE_ELEM(3103, 1130, US, DCM_AMIANNOTSEQUENCECOLOR_OLD, "AMI Annotation Color (RET)")
PRIVATE_ELEM(3103, 1150, CS, DCM_AMIANNOTSEQUENCELINESTYLE_OLD, "AMI Annotation Line Style (RET)")
PRIVATE_ELEM(3103, 1160, SQ, DCM_AMIANNOTSEQUENCEELEMENTS_OLD, "AMI Annotation Elements (RET)")
PRIVATE_ELEM(3103, 1170, SH, DCM_AMIANNOTSEQUENCELABEL_OLD, "AMI Annotation Label (RET)")
PRIVATE_ELEM(3103, 1180, PN, DCM_AMIANNOTSEQUENCECREATOR_OLD, "AMI Annotation Creator (RET)")
PRIVATE_ELEM(3103, 1190, PN, DCM_AMIANNOTSEQUENCEMODIFIERS_OLD, "AMI Annotation Modifiers (RET)")
PRIVATE_ELEM(3103, 11A0, DA, DCM_AMIANNOTSEQUENCECREATIONDATE_OLD, "AMI Annotation Creation Date (RET)")
PRIVATE_ELEM(3103, 11B0, TM, DCM_AMIANNOTSEQUENCECREATIONTIME_OLD, "AMI Annotation Creation Time (RET)")
PRIVATE_ELEM(3103, 11C0, DA, DCM_AMIANNOTSEQUENCEMODIFYDATES_OLD, "AMI Annotation Modification Dates (RET)")
PRIVATE_ELEM(3103, 11D0, TM, DCM_AMIANNOTSEQUENCEMODIFYTIMES_OLD, "AMI Annotation Mofification Times (RET)")
PRIVATE_ELEM(3103, 11E0, US, DCM_AMIANNOTSEQUENCEFRAMENUMBER_OLD, "AMI Annotation Frame Number (RET)")

DATA_ELEM(3103, 0010, LO, "AMI Sequence Annotations_02")
PRIVATE_ELEM(3103, 1010, CS, DCM_AMIANNOTSEQUENCETYPE, "AMI Annotation Sequence (RET)")
PRIVATE_ELEM(3103, 1020, UI, DCM_AMIANNOTSEQUENCEUID, "AMI Annotation UID (RET)")
PRIVATE_ELEM(3103, 1030, US, DCM_AMIANNOTSEQUENCECOLOR, "AMI Annotation Color (RET)")
PRIVATE_ELEM(3103, 1050, CS, DCM_AMIANNOTSEQUENCELINESTYLE, "AMI Annotation Line Style (RET)")
PRIVATE_ELEM(3103, 1060, SQ, DCM_AMIANNOTSEQUENCEELEMENTS, "AMI Annotation Elements (RET)")
PRIVATE_ELEM(3103, 1070, SH, DCM_AMIANNOTSEQUENCELABEL, "AMI Annotation Label (RET)")
PRIVATE_ELEM(3103, 1080, PN, DCM_AMIANNOTSEQUENCECREATOR, "AMI Annotation Creator (RET)")
PRIVATE_ELEM(3103, 1090, PN, DCM_AMIANNOTSEQUENCEMODIFIERS, "AMI Annotation Modifiers (RET)")
PRIVATE_ELEM(3103, 10A0, DA, DCM_AMIANNOTSEQUENCECREATIONDATE, "AMI Annotation Creation Date (RET)")
PRIVATE_ELEM(3103, 10B0, TM, DCM_AMIANNOTSEQUENCECREATIONTIME, "AMI Annotation Creation Time (RET)")
PRIVATE_ELEM(3103, 10C0, DA, DCM_AMIANNOTSEQUENCEMODIFYDATES, "AMI Annotation Modification Dates (RET)")
PRIVATE_ELEM(3103, 10D0, TM, DCM_AMIANNOTSEQUENCEMODIFYTIMES, "AMI Annotation Modification Times (RET)")
PRIVATE_ELEM(3103, 10E0, US, DCM_AMIANNOTSEQUENCEFRAMENUMBER, "AMI Annotation Frame Number (RET)")

DATA_ELEM(3105, 0010, LO, "AMI Sequence AnnotElements_01")
PRIVATE_ELEM(3105, 1010, DS, DCM_AMIANNOTELEMENTSEQPOSITION, "AMI Annotation Element Position")
PRIVATE_ELEM(3105, 1020, LT, DCM_AMIANNOTELEMENTSEQTEXT, "AMI Annotation Element Text")


DATA_ELEM(3107, 0010, LO, "AMI ImageTransform_01")
PRIVATE_ELEM(3107, 1010, DS, DCM_AMITRANSMATRIX, "AMI Transformation Matrix (RET)")
PRIVATE_ELEM(3107, 1020, DS, DCM_AMICENTEROFFSET, "AMI Center Offset (RET)")
PRIVATE_ELEM(3107, 1030, DS, DCM_AMIMAGNIFICATION, "AMI Magnification (RET)")
PRIVATE_ELEM(3107, 1040, CS, DCM_AMIMAGNIFICATIONTYPE, "AMI Magnification Type (RET)")
PRIVATE_ELEM(3107, 1050, DS, DCM_AMIDISPLAYAREA, "AMI Displayed Area (RET)")
PRIVATE_ELEM(3107, 1060, DS, DCM_AMICALIBRATIONFACTOR, "AMI Calibration Factor (RET)")

DATA_ELEM(3107, 0011, LO, "AMI ImageContextExt_01")
PRIVATE_ELEM(3107, 11A0, CS, DCM_AMIWINDOWFUNCTION, "AMI Window Function (RET)")
PRIVATE_ELEM(3107, 11B0, DS, DCM_AMIWINDOWSLOPE, "AMI Window Slope (RET)")


DATA_ELEM(3109, 0010, LO, "Applicare/RadWorks/Version 5.0")
PRIVATE_ELEM(3109, 1001, ST, DCM_WORKLISTFILENAME, "<internal>")
PRIVATE_ELEM(3109, 1002, SH, DCM_AMI_STATUS, "NEW/SEEN Status")
PRIVATE_ELEM(3109, 1003, CS, DCM_AMI_DELETELOCK, "Delete Lock")				// Flag indicating study is locked. Defined values: 'L' or ' '
PRIVATE_ELEM(3109, 1004, CS, DCM_AMI_STATUS2_RETIRED, "<internal>")
PRIVATE_ELEM(3109, 1005, CS, DCM_AMI_STATUS3_RETIRED, "<internal>")
PRIVATE_ELEM(3109, 1006, CS, DCM_AMI_STATUS4_RETIRED, "<internal>")
PRIVATE_ELEM(3109, 1007, UL, DCM_AMI_STATUSBITS_RETIRED, "<internal>")
PRIVATE_ELEM(3109, 1008, LO, DCM_AMI_ORIGIN, "Receive Origin")
PRIVATE_ELEM(3109, 1009, LO, DCM_AMI_FOLDER, "Folder")
PRIVATE_ELEM(3109, 100A, DA, DCM_AMI_RECEIVEDATE, "Receive Date")
PRIVATE_ELEM(3109, 100B, TM, DCM_AMI_RECEIVETIME, "Receive Time")
PRIVATE_ELEM(3109, 100C, CS, DCM_AMI_PRIOR, "Prior")
PRIVATE_ELEM(3109, 100D, CS, DCM_AMI_STAT, "STAT Study")						// Flag indicating study is STAT. Defined values 'STAT' or 'ROUTINE'
PRIVATE_ELEM(3109, 100E, CS, DCM_AMI_KEY, "<internal>")						// Flag indicating study/image is KEY. Defined values 'KEY' or ' '
PRIVATE_ELEM(3109, 1010, CS, DCM_AMI_LOCALSTUDY, "<internal>")
PRIVATE_ELEM(3109, 1011, LO, DCM_AMI_RESULT_MSG, "<internal>")
PRIVATE_ELEM(3109, 1012, LO, DCM_AMI_CURRENT_USER, "<internal>")
PRIVATE_ELEM(3109, 1013, DA, DCM_AMI_SYSTEM_DATE, "<internal>")
PRIVATE_ELEM(3109, 1014, TM, DCM_AMI_SYSTEM_TIME, "<internal>")
PRIVATE_ELEM(3109, 1019, LO, DCM_AMI_WORKLISTNAME, "<internal>")			// Refers to the name of the Worklist
PRIVATE_ELEM(3109, 1020, UI, DCM_AMI_WORKLISTUID, "<internal>")				// Refers to the UID of the Worklist
PRIVATE_ELEM(3109, 1021, CS, DCM_AMI_HOSTNAME, "<internal>")	
PRIVATE_ELEM(3109, 1022, AE, DCM_AMI_DICOM_AE_TITLE, "<internal>")
PRIVATE_ELEM(3109, 1023, US, DCM_AMI_DICOM_PORT_NUMBER, "<internal>")
PRIVATE_ELEM(3109, 1024, LO, DCM_AMI_DESTINATION_NAME, "<internal>")
PRIVATE_ELEM(3109, 1025, LO, DCM_AMI_ORIGIN_NAME, "<internal>")				// AMI origin name
PRIVATE_ELEM(3109, 1026, UI, DCM_AMI_MOD_STUDYINSTANCEUID, "<internal>")		// Syudy instance uid generated by modality
PRIVATE_ELEM(3109, 1027, SQ, DCM_AMI_EXAM_ROUTING, "<internal>")				// Sequence (AE, Host, Port, Stor. Comm.)
PRIVATE_ELEM(3109, 1028, LO, DCM_AMI_NOTIFICATION_COMMENTS, "<internal>")
PRIVATE_ELEM(3109, 1029, LO, DCM_AMI_TRANSACTION_COMMENTS, "<internal>")
PRIVATE_ELEM(3109, 102A, LO, DCM_AMI_FLAG_SEND, "Send Flag")
PRIVATE_ELEM(3109, 102B, LO, DCM_AMI_FLAG_PRINT, "Print Flag")
PRIVATE_ELEM(3109, 102C, LO, DCM_AMI_FLAG_ARCHIVE, "Archive Flag")
PRIVATE_ELEM(3109, 1030, LO, DCM_AMI_REQ_FACILITY_NAME, "<internal>")			// Requesting Facility Name (used with ADAC)
PRIVATE_ELEM(3109, 1031, CS, DCM_AMI_REQ_PROCEDURE_NAME, "<internal>")		// Requesting Procedure Name (used with ADAC)
PRIVATE_ELEM(3109, 1032, CS, DCM_AMI_REQ_PROCEDURE_CODE, "<internal>")		// Requesting Procedure Code (used with ADAC)
PRIVATE_ELEM(3109, 1033, CS, DCM_AMI_STORAGE_COMMIT, "Request Storage Commitment")			// Flag that indicates if storage commitment should be requested
PRIVATE_ELEM(3109, 1034, CS, DCM_AMI_COMPRESSION, "Requested Compression")				// Private Tag (CS) added to a DICOM C-MOVE request
																// defined values: <none> - standard uncompressed DICOM
PRIVATE_ELEM(3109, 1036, LO, DCM_AMI_UPDATEORIGIN, "<internal>")				// Origin of update (used by Local Worklist)

																//					JPEG:<qfactor> - qfactor: LL (lossless), 10, 20..90
PRIVATE_ELEM(3109, 1035, SQ, DCM_AMI_STUDY_SEQ, "<internal>")					// Study sequence for replies to PATIENT level queries
//PRIVATE_ELEM(3109, 1036, DCM_AMI_UPDATEORIGIN)					// Origin of update (used by Local Worklist)
PRIVATE_ELEM(3109, 1037, UI, DCM_AMI_REPLACEDSTUDYUID, "<internal>")			// Study UID that is being replaced
PRIVATE_ELEM(3109, 1038, SH, DCM_AMI_TEACHING_ACR, "<internal>")				// ACR code for teaching "folder" worklists
PRIVATE_ELEM(3109, 1039, SH, DCM_AMI_TEACHING_SIC, "<internal>")				// Special Interest Code (hospital defined code used for teaching worklist)

PRIVATE_ELEM(3109, 1040, IS, DCM_AMI_REAL_STUDYRELATEDIMAGES, "<internal>")	// Number of Study Related Images (Study header)"
PRIVATE_ELEM(3109, 1041, CS, DCM_AMI_STUDYLOCKED, "<internal>")				// Study locked
PRIVATE_ELEM(3109, 1042, CS, DCM_AMI_WORKSTATION, "<internal>")				// contains workstation name
PRIVATE_ELEM(3109, 1043, CS, DCM_AMI_ARCHIVESTATUS, "Archive Status")		// archive status { <Empty>, "ARCHIVED" }

PRIVATE_ELEM(3109, 10EE, UI, DCM_AMI_INTERNAL_LIST_UID, "<internal>")			// Internal tag to set list UID
PRIVATE_ELEM(3109, 10EF, CS, DCM_AMI_ACTION, "<internal>")					// Internal tag { ADD, REMOVE, CHANGE }

DATA_ELEM(3109, 0011, LO, "AMI ImageContext_01")
PRIVATE_ELEM(3109, 1110, CS, DCM_AMIWINDOWINVERT, "AMI Window Invert (RET)")
PRIVATE_ELEM(3109, 1120, IS, DCM_AMIWINDOWCENTER, "AMI Window Center (RET)")
PRIVATE_ELEM(3109, 1130, IS, DCM_AMIWINDOWWIDTH, "AMI Window Widith (RET)")
PRIVATE_ELEM(3109, 1140, CS, DCM_AMIPIXELASPECTRATIOSWAP, "AMI Pixel Aspect Ratio Swap (RET)")
PRIVATE_ELEM(3109, 1150, CS, DCM_AMIENABLEAVERAGING, "AMI Enable Averaging (RET)")
PRIVATE_ELEM(3109, 1160, CS, DCM_AMIQUALITY, "AMI Quality (RET)")
PRIVATE_ELEM(3109, 1170, CS, DCM_AMIANNOTATION, "AMI Viewport Annotation Level (RET)")
PRIVATE_ELEM(3109, 1180, CS, DCM_AMIIMAGEANNOTATION, "AMI Show Image Annotation (RET)")
PRIVATE_ELEM(3109, 1190, CS, DCM_AMIOVERLAY, "AMI Show Image Overlay (RET)")

DATA_ELEM(3109, 0012, LO, "Applicare/RadWorks/Version 6.0/Summary")
//PRIVATE_ELEM(3109, 1201, SH, DCM_SUMMARY_STATUS) - is called DCM_AMI_STATUS
//PRIVATE_ELEM(3109, 1211, ST, DCM_SUMMARY_ORGSITENAME) - is called DCM_AMI_ORIGIN
PRIVATE_ELEM(3109, 1212, ST, DCM_SUMMARY_ORGSITEDESCR, "Receive Origin Description")
//PRIVATE_ELEM(3109, 1215, DA, DCM_SUMMARY_RECEIVEDATE) - is called DCM_AMI_RECEIVEDATE
//PRIVATE_ELEM(3109, 1216, TM, DCM_SUMMARY_RECEIVETIME) - is called DCM_AMI_RECEIVETIME

DATA_ELEM(3115, 0017, LO, "http://www.gemedicalsystems.com/it_solutions/rad_pacs/")
PRIVATE_ELEM(3115, 1701, UT, DCM_NODEREF_XML, "Reference to pacs study")
PRIVATE_ELEM(3115, 1702, UT, DCM_IMAGEREF_XML, "Reference to pacs image")
PRIVATE_ELEM(3115, 1703, CS, DCM_EXAMNOTES_FLAG, "Pacs examnotes flag")

DATA_ELEM(3117, 0010, LO, "http://www.gemedicalsystems.com/it_solutions/orthoview/2.1")
PRIVATE_ELEM(3117, 1010, DT, DCM_ORTHOVIEW_SESSION_DATE, "OrthoView Session Date/Time")
PRIVATE_ELEM(3117, 1020, PN, DCM_ORTHOVIEW_SESSION_CREATOR, "OrthoView Session Creator")
PRIVATE_ELEM(3117, 1030, CS, DCM_ORTHOVIEW_SESSION_COMPLETION_FLAG, "OrthoView Session Completion Flag")
PRIVATE_ELEM(3117, 1040, SQ, DCM_ORTHOVIEW_FILE_SEQUENCE, "OrthoView File Sequence")
PRIVATE_ELEM(3117, 1050, ST, DCM_ORTHOVIEW_FILE_NAME, "OrthoView File Name")
PRIVATE_ELEM(3117, 1060, OB, DCM_ORTHOVIEW_FILE_CONTENT, "OrthoView File Content")

DATA_ELEM(3118, 0010, LO, "http://www.gemedicalsystems.com/it_solutions/bamwallthickness/1.0")
PRIVATE_ELEM(3118, 1010, DT, DCM_BAM_SESSION_DATE, "BAM WallThickness Session Date/Time")
PRIVATE_ELEM(3118, 1020, PN, DCM_BAM_SESSION_CREATOR, "BAM WallThickness Session Creator")
PRIVATE_ELEM(3118, 1030, CS, DCM_BAM_SESSION_COMPLETION_FLAG, "BAM WallThickness Session Completion Flag")
PRIVATE_ELEM(3118, 1040, SQ, DCM_BAM_FILE_SEQUENCE, "BAM WallThickness File Sequence")
PRIVATE_ELEM(3118, 1050, ST, DCM_BAM_FILE_NAME, "BAM WallThickness File Name")
PRIVATE_ELEM(3118, 1060, OB, DCM_BAM_FILE_CONTENT, "BAM WallThickness File Content")

DATA_ELEM(3111, 0010, LO, "AMI StudyExtensions_01")
PRIVATE_ELEM(3111, 1001, UL, DCM_AMI_LAST_RELEASED_ANNOT, "AMI Last Released Annot Label (RET)")		

DATA_ELEM(3111, 0011, LO, "RadWorksTBR")		
PRIVATE_ELEM(3111, 1102, CS, DCM_AMI_COMPRESSIONTYPE, "AMI Compression Type (RET)")
PRIVATE_ELEM(3111, 11FF, SQ, DCM_AMI_QUERY_RESULT, "<internal>")

//-------------------- RadStore -----------------------------
DATA_ELEM(3113, 0010, LO, "Applicare/RadStore/Version 1.0")
DATA_ELEM(3113, 1001, SL, "OBSOLETE")
DATA_ELEM(3113, 1002, SL, "Id1")
DATA_ELEM(3113, 1003, SL, "Id2")
DATA_ELEM(3113, 1004, SL, "Id3")

DATA_ELEM(3113, 1011, LO, "OBSOLETE")
DATA_ELEM(3113, 1012, CS, "State") 					// image archiving state
DATA_ELEM(3113, 1013, DT, "DateLastModified")
DATA_ELEM(3113, 1014, DT, "DateLastAccessed")
DATA_ELEM(3113, 1015, CS, "OBSOLETE")
DATA_ELEM(3113, 1016, FD, "ByteSize")
DATA_ELEM(3113, 1017, LO, "LibraryId")
DATA_ELEM(3113, 1018, LO, "Pathnames")
DATA_ELEM(3113, 1019, LO, "DriverPath")
DATA_ELEM(3113, 101A, LO, "Source")
DATA_ELEM(3113, 101B, LO, "Destination")
DATA_ELEM(3113, 101C, SL, "MediumId")
DATA_ELEM(3113, 101D, LO, "ArchiveId")
DATA_ELEM(3113, 101E, LO, "Origin")
DATA_ELEM(3113, 1021, SL, "Version")
DATA_ELEM(3113, 1022, SL, "OBSOLETE")
DATA_ELEM(3113, 1023, ST, "InstanceFileLocation")

DATA_ELEM(3113, 1031, IS, "OBSOLETE")
DATA_ELEM(3113, 1032, IS, "OBSOLETE")
DATA_ELEM(3113, 1033, IS, "OBSOLETE")

// media information
DATA_ELEM(3113, 1035, LO, "ImageMediumLocation")
DATA_ELEM(3113, 1036, LO, "ImageMediumLabel")
DATA_ELEM(3113, 1037, CS, "ImageMediumState")
DATA_ELEM(3113, 1038, LO, "SeriesMediumLocation")
DATA_ELEM(3113, 1039, LO, "SeriesMediumLabel")
DATA_ELEM(3113, 103A, CS, "SeriesMediumState")
DATA_ELEM(3113, 103B, LO, "StudyMediumLocation")
DATA_ELEM(3113, 103C, LO, "StudyMediumLabel")
DATA_ELEM(3113, 103D, CS, "StudyMediumState")

// archiving states
DATA_ELEM(3113, 1052, CS, "StudyState")				// binary composition of image states
DATA_ELEM(3113, 1053, CS, "SeriesState")			// binary composition of image states
DATA_ELEM(3113, 1055, CS, "ImageStateText")			// textual description of image state
DATA_ELEM(3113, 1056, CS, "SeriesStateText")		// textual description combined series state
DATA_ELEM(3113, 1057, CS, "StudyStateText")			// textual description combined study state

DATA_ELEM(3113, 1060, DT, "Expiration")				// determines lifetime of internal worklist items (RadStore-PRouter)
DATA_ELEM(3113, 1069, AT, "DeletedTags")

//---------------- Workstation printing --------------------------------
DATA_ELEM(4101, 0010, LO, "Applicare/Print/Version 5.1")
PRIVATE_ELEM(4101, 1001, UL, DCM_PRINT_MASKSTATE, "<internal>")
PRIVATE_ELEM(4101, 1002, SQ, DCM_PRINT_ANNOTS, "<internal>")
PRIVATE_ELEM(4101, 1003, LO, DCM_PRINT_FONT, "<internal>")
PRIVATE_ELEM(4101, 1004, UL, DCM_PRINT_FONTSIZE, "<internal>")
PRIVATE_ELEM(4101, 1005, FD, DCM_PRINT_FONTRELSIZE, "<internal>")
PRIVATE_ELEM(4101, 1006, US, DCM_PRINT_OVERLAY, "<internal>")
PRIVATE_ELEM(4101, 1007, US, DCM_PRINT_PIXELREP, "<internal>")
PRIVATE_ELEM(4101, 1008, US, DCM_PRINT_ANNOTATION_LEVEL, "<internal>")
PRIVATE_ELEM(4101, 1009, US, DCM_PRINT_SHOW_CALIPER, "<internal>")

//---------------- Workstation file format------------------------------
DATA_ELEM(4103, 0010, LO, "Applicare/RadWorks/Version 6.0")
PRIVATE_ELEM(4103, 1001, AT, DCM_FFMT_NONEXISTENTTAGS, "Internal: non-existent tags")
PRIVATE_ELEM(4103, 1002, UI, DCM_FFMT_NONEXISTENTOBJECTS, "Internal: non-existent objects")

//---------------- Workstation annotations------------------------------
DATA_ELEM(4105, 0010, LO, "Applicare/RadWorks/Version 6.0")
PRIVATE_ELEM(4105, 1001, CS, DCM_ANNOT_TYPE, "Annotation Type")
PRIVATE_ELEM(4105, 1002, DS, DCM_ANNOT_VALUE, "Annotation Value")
PRIVATE_ELEM(4105, 1003, UI, DCM_ANNOT_CUTLINE_IMAGE_UID, "Cutline Image UID")
PRIVATE_ELEM(4105, 1004, UI, DCM_ANNOT_CUTLINE_SET_UID, "Cutline Set UID")
PRIVATE_ELEM(4105, 1005, US, DCM_ANNOT_COLOR, "Annotation Color")
PRIVATE_ELEM(4105, 1006, CS, DCM_ANNOT_LINESTYLE, "Annotation Line Style")
PRIVATE_ELEM(4105, 1007, SH, DCM_ANNOT_LABEL, "Annotation Label")
PRIVATE_ELEM(4105, 1008, PN, DCM_ANNOT_CREATOR, "Annotation Creator")
PRIVATE_ELEM(4105, 1009, DA, DCM_ANNOT_CREATIONDATE, "Annotation Creation Date")
PRIVATE_ELEM(4105, 100A, TM, DCM_ANNOT_CREATIONTIME, "Annotation Creation Time")
PRIVATE_ELEM(4105, 100B, SQ, DCM_ANNOT_SEQUENCE_MODIFICATION, "Annotation Modification Sequence")
PRIVATE_ELEM(4105, 100C, PN, DCM_ANNOT_MODIFIER, "Annotation Modifier")
PRIVATE_ELEM(4105, 100D, DA, DCM_ANNOT_MODIFICATIONDATE, "Annotation Modification Date")
PRIVATE_ELEM(4105, 100E, TM, DCM_ANNOT_MODIFICATIONTIME, "Annotation Modification Time")

PRIVATE_ELEM(4105, 100F, LO, DCM_ANNOT_PALETTECOLORLUT_NAME, "Palette Color LUT Name")

PRIVATE_ELEM(4105, 1010, US, DCM_ANNOT_NUMBER, "Annotation Number")

//---------------- Presentation states----------------------
DATA_ELEM(4107, 0010, LO, "Applicare/RadWorks/Version 6.0")
PRIVATE_ELEM(4107, 1001, SQ, DCM_PRESSTATE_PALETTECOLORLUT, "Requested Palette Color LUT")

//---------------- Centricity Radiology Web Mammography ----------------------
DATA_ELEM(4109, 0010, LO, "Applicare/Centricity Radiology Web/Version 1.0")
PRIVATE_ELEM(4109, 1001, SH, DCM_MG_LATERALITY,		"Mammography Laterality")
PRIVATE_ELEM(4109, 1002, SH, DCM_MG_VIEWNAME,		"Mammography View Name")
PRIVATE_ELEM(4109, 1003, SH, DCM_MG_VIEWMODIFIER,	"Mammography View Modifier")

//---------------- Centricity Radiology Web ----------------------
DATA_ELEM(4111, 0010, LO, "Applicare/Centricity Radiology Web/Version 2.0")
PRIVATE_ELEM(4111, 1001, CS, DCM_AMI_SECONDARY_SPINE_LABEL, "Secondary Spine Label")
PRIVATE_ELEM(4111, 1002, IS, DCM_AMI_PRESENTATIONSTATE_ADDITIONALTAGS, "Additional tags for Presentation State")		

//---------------- GEMS-IT Centricity RA600 Query ------------------------------
DATA_ELEM(4113, 0010, LO, "GEMS-IT/Centricity RA600/7.0")
PRIVATE_ELEM(4113, 1010, UI, DCM_NUMBEROFIMAGESINSTUDY, "Number of images in study")

//---------------- GE Pathspeed Specific-----------------------------
DATA_ELEM(0009, 0010, LO, "GEIIS")
PRIVATE_ELEM(0009, 1010, SQ, DCM_GEIIS_THUMBNAIL_SEQUENCE, "GE IIS Thumbnail Sequence")

//---------------- GE Pathspeed Specific-----------------------------
DATA_ELEM(7FD1, 0010, LO, "GEIIS")
PRIVATE_ELEM(7FD1, 1010, UL, DCM_GEIIS_COMPRESSION_ID, "GE IIS Compression ID")
PRIVATE_ELEM(7FD1, 1020, UL, DCM_GEIIS_MULTIFRAME_OFFSETS, "GE IIS Multiframe Offsets")

//---------------- GE Specific---------------------------------------
DATA_ELEM(0045, 0010, LO, "GE LUT Asymmetry Parameter")
PRIVATE_ELEM(0045, 1067, DS, DCM_GE_LUT_ASYMMETRY, "LUT Assymetry")

//---------------- Workflow Specific------------------------------
DATA_ELEM(3113, 0020, LO, "Applicare/Workflow/Version 1.0")
PRIVATE_ELEM(3113, 2001, CS, OrderControl, "<internal>") // From Hl7
PRIVATE_ELEM(3113, 2010, SH, ScheduledActionItemCodeValue, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2011, SH, ScheduledActionItemCodingSchemeDesignator, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2012, LO, ScheduledActionItemCodeMeaning, "<internal>") // To flat out hierarchical sequence 

PRIVATE_ELEM(3113, 2015, SH, RequestedActionItemCodeValue, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2016, SH, RequestedActionItemCodingSchemeDesignator, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2017, LO, RequestedActionItemCodeMeaning, "<internal>") // To flat out hierarchical sequence 

PRIVATE_ELEM(3113, 2020, SH, PerformedActionItemCodeValue, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2021, SH, PerformedActionItemCodingSchemeDesignator, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2022, LO, PerformedActionItemCodeMeaning, "<internal>") // To flat out hierarchical sequence 

PRIVATE_ELEM(3113, 2025, SH, PerformedProcedureCodeValue, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2026, SH, PerformedProcedureCodingSchemeDesignator, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2027, LO, PerformedProcedureCodeMeaning, "<internal>") // To flat out hierarchical sequence 

PRIVATE_ELEM(3113, 2030, UI, ReferencedImageSOPClassUID, "<internal>") // To flat out hierarchical sequence 
PRIVATE_ELEM(3113, 2031, UI, ReferencedImageSOPInstanceUID, "<internal>") // To flat out hierarchical sequence 

// workflow integration dll
PRIVATE_ELEM(3113, 20E0, CS, LockedByHostname, "<internal>")	// hostname of the station that locked the worklist item
PRIVATE_ELEM(3113, 20E1, CS, LockedByUser, "<internal>")	// username of the NT user that locked the worklist item
PRIVATE_ELEM(3113, 20E2, CS, KfEditLockUser, "<internal>")  // Keyflow field for the exchange username of user that locked the worklist item

// --- GE DLX patient attributes
DATA_ELEM(0011, 0010, LO, "DLX_PATNT_01")
PRIVATE_ELEM(0011, 1001, LT, DCM_DLX_PAT_DOB, "patient DOB")

// --- GE DL (Innova) patient attributes
DATA_ELEM(0011, 0011, LO, "GEMS_DL_PATNT_01")
PRIVATE_ELEM(0011, 1180, UI, DCM_DL_PAT_INST_UID,       "Patient Instance Uid")
PRIVATE_ELEM(0011, 1181, IS, DCM_DL_PAT_LAST_STUDY_NUM, "Last Study Number")
PRIVATE_ELEM(0011, 1182, CS, DCM_DL_PAT_REPAIRED,       "Patient Repaired")
PRIVATE_ELEM(0011, 1183, CS, DCM_DL_PAT_LOCK_DEMO,      "Lock Demographics")

// --- GE DL (Innova) study attributes
DATA_ELEM(0015, 0010, LO, "GEMS_DL_STUDY_01")
PRIVATE_ELEM(0015, 1080, DS, DCM_DL_STUDY_DOSE,                     "Study Dose")
PRIVATE_ELEM(0015, 1081, DS, DCM_DL_STUDY_TOTAL_DAP,                "Study Total Dap")
PRIVATE_ELEM(0015, 1082, DS, DCM_DL_STUDY_FLUORO_DAP,               "Study Fluoro Dap")
PRIVATE_ELEM(0015, 1083, IS, DCM_DL_STUDY_FLUORO_TIME,              "Study Fluoro Time")
PRIVATE_ELEM(0015, 1084, DS, DCM_DL_STUDY_RECORD_DAP,               "Study Record Dap")
PRIVATE_ELEM(0015, 1085, IS, DCM_DL_STUDY_RECORD_TIME,              "Study Record Time")
PRIVATE_ELEM(0015, 1086, IS, DCM_DL_STUDY_LAST_XA_NUM,              "Last Xa Number")
PRIVATE_ELEM(0015, 1088, PN, DCM_DL_STUDY_DEF_OPERATOR_NAME,        "Default Operator Name")
PRIVATE_ELEM(0015, 1089, PN, DCM_DL_STUDY_DEF_PERF_PHYS_NAME,       "Default Performing Physician Name")
PRIVATE_ELEM(0015, 108A, CS, DCM_DL_STUDY_DEF_PATIENT_ORIENTATION,  "Default Patient Orientation")
PRIVATE_ELEM(0015, 108B, IS, DCM_DL_STUDY_LAST_SC_NUM,              "Last Sc Number")
PRIVATE_ELEM(0015, 108E, UI, DCM_DL_STUDY_COMMON_SERIES_INST_UID,   "Common Series Instance Uid")
PRIVATE_ELEM(0015, 108F, IS, DCM_DL_STUDY_NUM,                      "Study Number")

// --- GE DL (Innova) series attributes
DATA_ELEM(0015, 0011, LO, "GEMS_DL_SERIES_01")
PRIVATE_ELEM(0015, 1185, LO, DCM_DL_SERIES_FILE_NAME,   "Series File Name")
PRIVATE_ELEM(0015, 1187, IS, DCM_DL_SERIES_NUM_IMAGES,  "Number Of Images")
PRIVATE_ELEM(0015, 118C, CS, DCM_DL_SERIES_SENT_FLAG,   "Sent Flag")
PRIVATE_ELEM(0015, 118D, US, DCM_DL_SERIES_ITEM_LOCKED, "Item Locked")

// --- GE DLX series attributes
DATA_ELEM(0019, 0010, LO, "DLX_SERIE_01")
PRIVATE_ELEM(0019, 1001, DS, DCM_DLX_SERIES_ANGLE_VAL_1,                        "Angle Value 1")
PRIVATE_ELEM(0019, 1002, DS, DCM_DLX_SERIES_ANGLE_VAL_2,                        "Angle Value 2")
PRIVATE_ELEM(0019, 1003, DS, DCM_DLX_SERIES_ANGLE_VAL_3,                        "Angle Value 3")
PRIVATE_ELEM(0019, 1004, CS, DCM_DLX_SERIES_ANGLE_LABEL_1,                      "Angle Label 1")
PRIVATE_ELEM(0019, 1005, CS, DCM_DLX_SERIES_ANGLE_LABEL_2,                      "Angle Label 2")
PRIVATE_ELEM(0019, 1006, CS, DCM_DLX_SERIES_ANGLE_LABEL_,                       "Angle Label 3")
PRIVATE_ELEM(0019, 1007, ST, DCM_DLX_SERIES_ADX_PROC_NAME,                      "Adx Procedure Name")
PRIVATE_ELEM(0019, 1008, ST, DCM_DLX_SERIES_ADX_EXAM_NAME,                      "Adx Exam Name")
PRIVATE_ELEM(0019, 1009, SH, DCM_DLX_SERIES_ADX_PAT_SIZE,                       "Adx Patient Size")
PRIVATE_ELEM(0019, 100A, IS, DCM_DLX_SERIES_ADX_RECORD_VIEW,                    "Adx Record View")
PRIVATE_ELEM(0019, 1010, DS, DCM_DLX_SERIES_ADX_INJECTOR_DELAY,                 "Adx Injector Delay")
PRIVATE_ELEM(0019, 1011, CS, DCM_DLX_SERIES_ADX_AUTO_INJECT,                    "Adx Auto Inject")
PRIVATE_ELEM(0019, 1014, IS, DCM_DLX_SERIES_ADX_ACQ_MODE,                       "Adx Acq Mode")
PRIVATE_ELEM(0019, 1015, CS, DCM_DLX_SERIES_ADX_CAMERA_ROTATION_ENABLE,         "Adx Camera Rotation Enable")
PRIVATE_ELEM(0019, 1016, CS, DCM_DLX_SERIES_ADX_REVERSE_SWEEP,                  "Adx Reverse Sweep")
PRIVATE_ELEM(0019, 1017, IS, DCM_DLX_SERIES_USER_SPATIAL_FILTER_STRENGTH,       "User Spatial Filter Strength")
PRIVATE_ELEM(0019, 1018, IS, DCM_DLX_SERIES_USER_ZOOM_FACTOR,                   "User Zoom Factor")
PRIVATE_ELEM(0019, 1019, IS, DCM_DLX_SERIES_X_ZOOM,                             "X Zoom")
PRIVATE_ELEM(0019, 101A, IS, DCM_DLX_SERIES_Y_ZOOM,                             "Y Zoom")
PRIVATE_ELEM(0019, 101B, DS, DCM_DLX_SERIES_ADX_FOCUS,                          "Adx Focus")
PRIVATE_ELEM(0019, 101C, CS, DCM_DLX_SERIES_ADX_DOSE,                           "Adx Dose")
PRIVATE_ELEM(0019, 101D, IS, DCM_DLX_SERIES_SIDE_MARK,                          "Side Mark")
PRIVATE_ELEM(0019, 101E, IS, DCM_DLX_SERIES_PCT_LANDSCAPE,                      "Percent Landscape")
PRIVATE_ELEM(0019, 101F, DS, DCM_DLX_SERIES_ADX_EXPOSURE_DURATION,              "Adx Exposure Duration")
PRIVATE_ELEM(0019, 1020, SH, DCM_DLX_SERIES_IP_ADDRESS,                         "Ip Address")
PRIVATE_ELEM(0019, 1021, DS, DCM_DLX_SERIES_TABLE_VERTICAL_POS,                 "Table Vertical Position")
PRIVATE_ELEM(0019, 1022, DS, DCM_DLX_SERIES_TABLE_LONGITUDINAL_POS,             "Table Longitudinal Position")
PRIVATE_ELEM(0019, 1023, DS, DCM_DLX_SERIES_TABLE_LATERAL_POS,                  "Table Lateral Position")
PRIVATE_ELEM(0019, 1024, DS, DCM_DLX_SERIES_LAMBDA_CM_PINCUSHION_DISTORTION,    "Lambda cm Pincushion Distortion")
PRIVATE_ELEM(0019, 1025, DS, DCM_DLX_SERIES_SLOPE_LV_REGRESSION,                "Slope LV Regression")
PRIVATE_ELEM(0019, 1026, DS, DCM_DLX_SERIES_INTERCEPT_LV_REGRESSION,            "Intercept LV Regression")
PRIVATE_ELEM(0019, 1027, DS, DCM_DLX_SERIES_IMAGE_CHAIN_FWHM_PSF_MM_MIN,        "Image chain FWHM psf mm min")
PRIVATE_ELEM(0019, 1028, DS, DCM_DLX_SERIES_IMAGE_CHAIN_FWHM_PSF_MM_MAX,        "Image chain FWHM psf mm max")

// --- GE DL (Innova) image attributes
DATA_ELEM(0019, 0011, LO, "GEMS_DL_IMG_01")
PRIVATE_ELEM(0019, 110B, DS, DCM_DL_IMG_FOV_DIMENSION_DOUBLE,               "Fov Dimension Double")
PRIVATE_ELEM(0019, 1130, LO, DCM_DL_IMG_FILE_NAME,                          "Image File Name")
PRIVATE_ELEM(0019, 1131, IS, DCM_DL_IMG_DEF_SPATIAL_FILTER_FAMILY,          "Default Spatial Filter Family")
PRIVATE_ELEM(0019, 1132, IS, DCM_DL_IMG_DEF_SPATIAL_FILTER_STRENGTH,        "Default Spatial Filter Strength")
PRIVATE_ELEM(0019, 1133, DS, DCM_DL_IMG_MIN_SATURATION_DOSE,                "Min Saturation Dose")
PRIVATE_ELEM(0019, 1134, DS, DCM_DL_IMG_DETECTOR_GAIN,                      "Detector Gain")
PRIVATE_ELEM(0019, 1135, DS, DCM_DL_IMG_PATIENT_DOSE_LIMIT,                 "Patient Dose Limit")
PRIVATE_ELEM(0019, 1136, DS, DCM_DL_IMG_PREPROC_IMAGE_RATE_MAX,             "Preproc Image Rate Max")
PRIVATE_ELEM(0019, 1137, CS, DCM_DL_IMG_SENSOR_ROI_SHAPE,                   "Sensor Roi Shape")
PRIVATE_ELEM(0019, 1138, DS, DCM_DL_IMG_SENSOR_ROI_X_POS,                   "Sensor Roi x Position")
PRIVATE_ELEM(0019, 1139, DS, DCM_DL_IMG_SENSOR_ROI_Y_POS,                   "Sensor Roi y Position")
PRIVATE_ELEM(0019, 113A, DS, DCM_DL_IMG_SENSOR_ROI_X_SIZE,                  "Sensor Roi x Size")
PRIVATE_ELEM(0019, 113B, DS, DCM_DL_IMG_SENSOR_ROI_Y_SIZE,                  "Sensor Roi y Size")
PRIVATE_ELEM(0019, 113D, DS, DCM_DL_IMG_NOISE_SENSITIVITY,                  "Noise Sensitivity")
PRIVATE_ELEM(0019, 113E, DS, DCM_DL_IMG_SHARP_SENSITIVITY,                  "Sharp Sensitivity")
PRIVATE_ELEM(0019, 113F, DS, DCM_DL_IMG_CONTRAST_SENSITIVITY,               "Contrast Sensitivity")
PRIVATE_ELEM(0019, 1140, DS, DCM_DL_IMG_LAG_SENSITIVITY,                    "Lag Sensitivity")
PRIVATE_ELEM(0019, 1141, CS, DCM_DL_IMG_TUBE,                               "Tube")
PRIVATE_ELEM(0019, 1142, US, DCM_DL_IMG_DETECTOR_SIZE_ROWS,                 "Detector Size Rows")
PRIVATE_ELEM(0019, 1143, US, DCM_DL_IMG_DETECTOR_SIZE_COLS,                 "Detector Size Columns")
PRIVATE_ELEM(0019, 1144, DS, DCM_DL_IMG_MIN_OBJ_SIZE,                       "Min Object Size")
PRIVATE_ELEM(0019, 1145, DS, DCM_DL_IMG_MAX_OBJ_SIZE,                       "Max Object Size")
PRIVATE_ELEM(0019, 1146, DS, DCM_DL_IMG_MAX_OBJ_SPEED,                      "Max Object Speed")
PRIVATE_ELEM(0019, 1147, CS, DCM_DL_IMG_OBJ_BACK_MOTION,                    "Object Back Motion")
PRIVATE_ELEM(0019, 1148, UL, DCM_DL_IMG_EXPOSURE_TRAJECTORY_FAMILY,         "Exposure Trajectory Family")
PRIVATE_ELEM(0019, 1149, DS, DCM_DL_IMG_WINDOW_TIME_DURATION,               "Window Time Duration")
PRIVATE_ELEM(0019, 114A, CS, DCM_DL_IMG_POSITIONER_ANGLE_PRIMARY_MODE,      "Positioner Angle Display Mode")
PRIVATE_ELEM(0019, 114B, IS, DCM_DL_IMG_DETECTOR_ORIGIN,                    "Detector Origin")
PRIVATE_ELEM(0019, 114E, DS, DCM_DL_IMG_DEFAULT_BRIGHTNESS_CONTRAST,        "Default Brightness Contrast")
PRIVATE_ELEM(0019, 114F, DS, DCM_DL_IMG_USER_BRIGHTNESS_CONTRAST,           "User Brightness Contrast")
PRIVATE_ELEM(0019, 1150, IS, DCM_DL_IMG_SOURCE_SERIES_NUMBER,               "Source Series Number")
PRIVATE_ELEM(0019, 1151, IS, DCM_DL_IMG_SOURCE_IMAGE_NUMBER,                "Source Image Number")
PRIVATE_ELEM(0019, 1152, IS, DCM_DL_IMG_SOURCE_FRAME_NUMBER,                "Source Frame Number")
PRIVATE_ELEM(0019, 1153, UI, DCM_DL_IMG_SOURCE_SERIES_ITEM_ID,              "Source Series Item Id")
PRIVATE_ELEM(0019, 1154, UI, DCM_DL_IMG_SOURCE_IMAGE_ITEM_ID,               "Source Image Item Id")
PRIVATE_ELEM(0019, 1155, UI, DCM_DL_IMG_SOURCE_FRAME_ITEM_ID,               "Source Frame Item Id")
PRIVATE_ELEM(0019, 1180, DS, DCM_DL_IMG_DOSE,                               "Image Dose")
PRIVATE_ELEM(0019, 1181, US, DCM_DL_IMG_CALIBRATION_FRAME,                  "Calibration Frame")
PRIVATE_ELEM(0019, 1182, CS, DCM_DL_IMG_CALIBRATION_OBJ,                    "Calibration Object")
PRIVATE_ELEM(0019, 1183, DS, DCM_DL_IMG_CALIBRATION_OBJ_SIZE_MM,            "Calibration Object Size mm")
PRIVATE_ELEM(0019, 1184, FL, DCM_DL_IMG_CALIBRATION_FACTOR,                 "Calibration Factor")
PRIVATE_ELEM(0019, 1185, DA, DCM_DL_IMG_CALIBRATION_DATE,                   "Calibration Date")
PRIVATE_ELEM(0019, 1186, TM, DCM_DL_IMG_CALIBRATION_TIME,                   "Calibration Time")
PRIVATE_ELEM(0019, 1187, US, DCM_DL_IMG_CALIBRATION_ACCURACY,               "Calibration Accuracy")
PRIVATE_ELEM(0019, 1188, CS, DCM_DL_IMG_CALIBRATION_EXTENDED,               "Calibration Extended")
PRIVATE_ELEM(0019, 1189, US, DCM_DL_IMG_CALIBRATION_IMAGE_ORIG,             "Calibration Image Original")
PRIVATE_ELEM(0019, 118A, US, DCM_DL_IMG_CALIBRATION_FRAME_ORIG,             "Calibration Frame Original")
PRIVATE_ELEM(0019, 118B, US, DCM_DL_IMG_CALIBRATION_NUM_POINTS_UIF,         "Calibration Number Of Points Uif")
PRIVATE_ELEM(0019, 118C, US, DCM_DL_IMG_CALIBRATION_POINTS_ROW,             "Calibration Points Row")
PRIVATE_ELEM(0019, 118D, US, DCM_DL_IMG_CALIBRATION_POINTS_COL,             "Calibration Points Column")
PRIVATE_ELEM(0019, 118E, FL, DCM_DL_IMG_CALIBRATION_MAGNIFICATION_RATIO,    "Calibration Magnification Ratio")
PRIVATE_ELEM(0019, 118F, LO, DCM_DL_IMG_CALIBRATION_SW_VERSION,             "Calibration Sw Version")
PRIVATE_ELEM(0019, 1190, LO, DCM_DL_IMG_EXTEND_CALIBRATION_SW_VERSION,      "Extend Calibration Sw Version")
PRIVATE_ELEM(0019, 1191, IS, DCM_DL_IMG_CALIBRATION_RETURN_CODE,            "Calibration Return Code")
PRIVATE_ELEM(0019, 1192, DS, DCM_DL_IMG_DETECTOR_ROTATION_ANGLE,            "Detector Rotation Angle")
PRIVATE_ELEM(0019, 1193, CS, DCM_DL_IMG_SPATIAL_CHANGE,                     "Spatial Change")
PRIVATE_ELEM(0019, 1194, CS, DCM_DL_IMG_INCONSISTENT_FLAG,                  "Inconsistent Flag")
PRIVATE_ELEM(0019, 1195, CS, DCM_DL_IMG_SWEEP,                              "Image Sweep")
PRIVATE_ELEM(0019, 1196, CS, DCM_DL_IMG_INTERNAL_LABEL_IMAGE,               "Internal Label Image")
PRIVATE_ELEM(0019, 1197, DS, DCM_DL_IMG_ANGLE_1_INCREMENT,                  "Angle 1 Increment")
PRIVATE_ELEM(0019, 1198, DS, DCM_DL_IMG_ANGLE_2_INCREMENT,                  "Angle 2 Increment")
PRIVATE_ELEM(0019, 1199, DS, DCM_DL_IMG_ANGLE_3_INCREMENT,                  "Angle 3 Increment")
PRIVATE_ELEM(0019, 119A, DS, DCM_DL_IMG_SENSOR_FEEDBACK,                    "Sensor Feedback")
PRIVATE_ELEM(0019, 119B, CS, DCM_DL_IMG_GRID,                               "Grid")
PRIVATE_ELEM(0019, 119C, FL, DCM_DL_IMG_DEF_MASK_PIXEL_SHIFT,               "Default Mask Pixel Shift")
PRIVATE_ELEM(0019, 119D, CS, DCM_DL_IMG_APPLICABLE_REVIEW_MODE,             "Applicable Review Mode")
PRIVATE_ELEM(0019, 119E, DS, DCM_DL_IMG_LOG_LUT_CONTROL_POINTS,             "Log Lut Control Points")
PRIVATE_ELEM(0019, 119F, DS, DCM_DL_IMG_EXP_LUT_CONTROL_POINTS,             "Exp Lut Control Points")
PRIVATE_ELEM(0019, 11A0, DS, DCM_DL_IMG_ABD_VALUE,                          "ABD Value")
PRIVATE_ELEM(0019, 11A1, DS, DCM_DL_IMG_SUB_WINDOW_CENTER,                  "Sub Window Center")
PRIVATE_ELEM(0019, 11A2, DS, DCM_DL_IMG_SUB_WINDOW_WIDTH,                   "Sub Window Width")
PRIVATE_ELEM(0019, 11A3, DS, DCM_DL_IMG_ROTATION,                           "Image Rotation")
PRIVATE_ELEM(0019, 11A4, CS, DCM_DL_IMG_AUTO_INJECTION_ENABLED,             "Auto Injection Enabled")
PRIVATE_ELEM(0019, 11A5, CS, DCM_DL_IMG_INJECTION_PHASE,                    "Injection Phase")
PRIVATE_ELEM(0019, 11A6, DS, DCM_DL_IMG_INJECTION_DELAY,                    "Injection Delay")
PRIVATE_ELEM(0019, 11A7, IS, DCM_DL_IMG_REF_INJECTION_FRAME_NUM,            "Reference Injection Frame Number")
PRIVATE_ELEM(0019, 11A8, DS, DCM_DL_IMG_INJECTION_DURATION,                 "Injection Duration")
PRIVATE_ELEM(0019, 11A9, DS, DCM_DL_IMG_EPT,                                "EPT")
PRIVATE_ELEM(0019, 11AA, CS, DCM_DL_IMG_CAN_DOWNSCAN_512,                   "Can Downscan 512")
PRIVATE_ELEM(0019, 11AB, IS, DCM_DL_IMG_CURRENT_SPATIAL_FILTER_STRENGTH,    "Current Spatial Filter Strength")
PRIVATE_ELEM(0019, 11AC, DS, DCM_DL_IMG_BRIGHTNESS_SENSITIVITY,             "Brightness Sensitivity")
PRIVATE_ELEM(0019, 11AD, DS, DCM_DL_IMG_EXP_LUT_NOSUB_CONTROL_POINTS,       "Exp Lut NOSUB Control Points")

// --- GE DL (Innova) series attributes
DATA_ELEM(0019, 0012, LO, "GEMS_DL_SERIES_01")
PRIVATE_ELEM(0019, 124C, CS, DCM_DL_SERIES_INTERNAL_LABEL,  "internal label")
PRIVATE_ELEM(0019, 124D, CS, DCM_DL_SERIES_BROWSER_HIDE,    "browser hide")

// --- GE DL (Innova) image frame attributes
DATA_ELEM(0025, 0010, LO, "GEMS_DL_FRAME_01")
PRIVATE_ELEM(0025, 1002, IS, DCM_DL_FRAME_ID,                               "Frame Id")
PRIVATE_ELEM(0025, 1003, DS, DCM_DL_FRAME_DIST_SOURCE_TO_DETECTOR,          "Distance Source To Detector")
PRIVATE_ELEM(0025, 1004, DS, DCM_DL_FRAME_DIST_SOURCE_TO_PATIENT,           "Distance Source To Patient")
PRIVATE_ELEM(0025, 1005, DS, DCM_DL_FRAME_DIST_SOURCE_TO_SKIN,              "Distance Source To Skin")
PRIVATE_ELEM(0025, 1006, DS, DCM_DL_FRAME_POSITIONER_PRIMARY_ANGLE,         "Positioner Primary Angle")
PRIVATE_ELEM(0025, 1007, DS, DCM_DL_FRAME_POSITIONER_SECONDARY_ANGLE,       "Positioner Secondary Angle")
PRIVATE_ELEM(0025, 1008, IS, DCM_DL_FRAME_BEAM_ORIENTATION,                 "Beam Orientation")
PRIVATE_ELEM(0025, 1009, DS, DCM_DL_FRAME_LARM_ANGLE,                       "Larm Angle")
PRIVATE_ELEM(0025, 100A, SQ, DCM_DL_FRAME_SEQUENCE,                         "Frame Sequence")
PRIVATE_ELEM(0025, 100B, DS, DCM_DL_FRAME_TARGET_CNR,                       "Target Cnr")
PRIVATE_ELEM(0025, 1010, DS, DCM_DL_FRAME_PIVOT_ANGLE,                      "Pivot Angle")
PRIVATE_ELEM(0025, 101A, DS, DCM_DL_FRAME_ARC_ANGLE,                        "Arc Angle")
PRIVATE_ELEM(0025, 101B, DS, DCM_DL_FRAME_TABLE_VERTICAL_POS,               "Table Vertical Position")
PRIVATE_ELEM(0025, 101C, DS, DCM_DL_FRAME_TABLE_LONGITUDINAL_POS,           "Table Longitudinal Position")
PRIVATE_ELEM(0025, 101D, DS, DCM_DL_FRAME_TABLE_LATERAL_POS,                "Table Lateral Position")
PRIVATE_ELEM(0025, 101E, IS, DCM_DL_FRAME_BEAM_COVER_AREA,                  "Beam Cover Area")
PRIVATE_ELEM(0025, 101F, DS, DCM_DL_FRAME_KVP_ACTUAL,                       "Kvp Actual")
PRIVATE_ELEM(0025, 1020, DS, DCM_DL_FRAME_MAS_ACTUAL,                       "Mas Actual")
PRIVATE_ELEM(0025, 1021, DS, DCM_DL_FRAME_PW_ACTUAL,                        "Pw Actual")
PRIVATE_ELEM(0025, 1022, DS, DCM_DL_FRAME_KVP_COMMANDED,                    "Kvp Commanded")
PRIVATE_ELEM(0025, 1023, DS, DCM_DL_FRAME_MAS_COMMANDED,                    "Mas Commanded")
PRIVATE_ELEM(0025, 1024, DS, DCM_DL_FRAME_PW_COMMANDED,                     "Pw Commanded")
PRIVATE_ELEM(0025, 1025, CS, DCM_DL_FRAME_GRID,                             "Grid")
PRIVATE_ELEM(0025, 1026, DS, DCM_DL_FRAME_SENSOR_FEEDBACK,                  "Sensor Feedback")
PRIVATE_ELEM(0025, 1027, DS, DCM_DL_FRAME_TARGET_ENTRANCE_DOSE,             "Target Entrance Dose")
PRIVATE_ELEM(0025, 1028, DS, DCM_DL_FRAME_CNR_COMMANDED,                    "Cnr Commanded")
PRIVATE_ELEM(0025, 1029, DS, DCM_DL_FRAME_CONTRAST_COMMANDED,               "Contrast Commanded")
PRIVATE_ELEM(0025, 102A, DS, DCM_DL_FRAME_EPT_ACTUAL,                       "Ept Actual")
PRIVATE_ELEM(0025, 102B, IS, DCM_DL_FRAME_SPECTRAL_FILTER_ZNB,              "Spectral Filter Znb")
PRIVATE_ELEM(0025, 102C, DS, DCM_DL_FRAME_SPECTRAL_FILTER_WEIGHT,           "Spectral Filter Weight")
PRIVATE_ELEM(0025, 102D, DS, DCM_DL_FRAME_SPECTRAL_FILTER_DENSITY,          "Spectral Filter Density")
PRIVATE_ELEM(0025, 102E, IS, DCM_DL_FRAME_SPECTRAL_FILTER_THICKNESS,        "Spectral Filter Thickness")
PRIVATE_ELEM(0025, 102F, IS, DCM_DL_FRAME_SPECTRAL_FILTER_FILTER_STATUS,    "Spectral Filter Status")
PRIVATE_ELEM(0025, 1030, IS, DCM_DL_FRAME_FOV_DIMENSION,                    "Fov Dimension")
PRIVATE_ELEM(0025, 1033, IS, DCM_DL_FRAME_FOV_ORIGIN,                       "Fov Origin")
PRIVATE_ELEM(0025, 1034, IS, DCM_DL_FRAME_COLLIMATOR_LEFT_VERTICAL_EDGE,    "Collimator Left Vertical Edge")
PRIVATE_ELEM(0025, 1035, IS, DCM_DL_FRAME_COLLIMATOR_RIGHT_VERTICAL_EDGE,   "Collimator Right Vertical Edge")
PRIVATE_ELEM(0025, 1036, IS, DCM_DL_FRAME_COLLIMATOR_UP_HORIZONTAL_EDGE,    "Collimator Up Horizontal Edge")
PRIVATE_ELEM(0025, 1037, IS, DCM_DL_FRAME_COLLIMATOR_LOW_HORIZONTAL_EDGE,   "Collimator Low Horizontal Edge")
PRIVATE_ELEM(0025, 1038, IS, DCM_DL_FRAME_VERTICES_POLYGONAL_COLLIMATOR,    "Vertices Polygonal Collimator")
PRIVATE_ELEM(0025, 1039, IS, DCM_DL_FRAME_CONTOUR_FILTER_DISTANCE,          "Contour Filter Distance")
PRIVATE_ELEM(0025, 103A, UL, DCM_DL_FRAME_CONTOUR_FILTER_ANGLE,             "Contour Filter Angle")
PRIVATE_ELEM(0025, 103B, CS, DCM_DL_FRAME_TABLE_ROTATION_STATUS,            "Table Rotation Status")
PRIVATE_ELEM(0025, 103C, CS, DCM_DL_FRAME_INTERNAL_LABEL_FRAME,             "Internal Label Frame")

// --- GEMnet Image Vault 3.0 fields indicating wrapped non-DICOM data files
DATA_ELEM(0045, 0011, LO, "GEMS_IT_US_REPORT")
PRIVATE_ELEM(0045, 1111, OW, DCM_GEMSIT_US_VIVID_EXCEL_FILE,    "Vivid excel file")
PRIVATE_ELEM(0045, 1112, OW, DCM_GEMSIT_US_VIVID_CHM_FILE,      "Vivid CHM file")
PRIVATE_ELEM(0045, 1113, OW, DCM_GEMSIT_US_VIVID_PDF_FILE,      "Vivid PDF file")

// --- Centricity Cardiology Image Management System 3.0
DATA_ELEM(0087, 0010, LO, "1.2.840.113708.794.1.1.2.0")
PRIVATE_ELEM(0087, 1010, CS, DCM_GEMSIT_IMS_MEDIA_TYPE,              "Media Type")
PRIVATE_ELEM(0087, 1020, CS, DCM_GEMSIT_IMS_MEDIA_LOCATION,          "Media Location")
PRIVATE_ELEM(0087, 1030, ST, DCM_GEMSIT_IMS_STORAGE_FILE_ID,         "Storage File ID")
PRIVATE_ELEM(0087, 1040, DS, DCM_GEMSIT_IMS_STUDY_OR_IMAGE_SIZE,     "Study or Image Size in MB")
PRIVATE_ELEM(0087, 1050, IS, DCM_GEMSIT_IMS_ESTIMATED_RETRIEVE_TIME, "Estimated Retrieve Time")
